(module Elabdev:Linx_ANT-868-SP_38x98mm (layer F.Cu) (tedit 5F57B566)
  (descr "868MHz Chip RF Antenna 1,1dBi Solder Surface Mount")
  (tags "antenna lora subghz subgigaherz")
  (attr smd)
  (fp_text reference REF** (at 17 -50) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Linx_ANT-868-SP_38x98mm (at -10 -50) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -19.43 -49.275) (end -19.43 49.275) (layer F.SilkS) (width 0.15))
  (fp_line (start -19.43 49.275) (end 19.43 49.275) (layer F.SilkS) (width 0.15))
  (fp_line (start 19.43 49.275) (end 19.43 -49.275) (layer F.SilkS) (width 0.15))
  (fp_line (start 19.43 -49.275) (end -19.43 -49.275) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy 18.925 48.77) (xy -18.925 48.77) (xy -18.925 -34.8) (xy 18.925 -34.8)) (layer B.Fab) (width 0.1))
  (fp_text user "Counterpoise copper plane " (at 0 0) (layer Cmts.User)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (fp_poly (pts (xy 13.97 -34.8) (xy -13.97 -34.8) (xy -13.97 -48.5) (xy 13.97 -48.5)) (layer F.Fab) (width 0.1))
  (fp_text user "Antenna chip" (at 0 -42) (layer Cmts.User)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (pad 1 smd rect (at -12.7 -34.8) (size 2.03 2.54) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -7.62 -34.8) (size 2.03 2.54) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.54 -34.8) (size 2.03 2.54) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.54 -34.8) (size 2.03 2.54) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 7.62 -34.8) (size 2.03 2.54) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 12.7 -34.8) (size 2.03 2.54) (layers F.Cu F.Paste F.Mask))
  (pad 2 thru_hole circle (at 12.7 -32.5) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
  (pad 2 smd rect (at 12.7 -33.175) (size 0.2 1) (layers F.Cu F.Mask))
  (pad 2 smd rect (at 7.62 -33.175) (size 0.2 1) (layers F.Cu F.Mask))
  (pad 2 smd rect (at 2.54 -33.175) (size 0.2 1) (layers F.Cu F.Mask))
  (pad 2 smd rect (at -2.54 -33.175) (size 0.2 1) (layers F.Cu F.Mask))
  (pad 2 smd rect (at -7.62 -33.175) (size 0.2 1) (layers F.Cu F.Mask))
  (pad 2 thru_hole circle (at 7.62 -32.5) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.54 -32.5) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -2.54 -32.5) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -7.62 -32.5) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
)
