(module Elabdev:Millmax_Pogopin_1x4_P2.54mm (layer F.Cu) (tedit 5F4D6FA6)
  (attr smd)
  (fp_text reference REF** (at 3 -2.5 unlocked) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Millmax_Pogopin_1x4_P2.54mm (at 0 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5.325 -1.5) (end -5.325 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.325 1.5) (end 5.325 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.325 1.5) (end 5.325 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.325 -1.5) (end -5.325 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.08 -1.27) (end -5.08 -1.27) (layer F.Fab) (width 0.15))
  (fp_line (start 5.08 1.27) (end 5.08 -1.27) (layer F.Fab) (width 0.15))
  (fp_line (start -5.08 1.27) (end 5.08 1.27) (layer F.Fab) (width 0.15))
  (fp_line (start -5.08 -1.27) (end -5.08 1.27) (layer F.Fab) (width 0.15))
  (fp_poly (pts (xy -5.325 -0.3) (xy -5.325 -1.5) (xy -4.125 -1.5)) (layer F.SilkS) (width 0.1))
  (pad 4 smd circle (at 3.81 0) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd circle (at 1.27 0) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd circle (at -1.27 0) (size 2 2) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd circle (at -3.81 0) (size 2 2) (layers F.Cu F.Paste F.Mask))
)
