(module Elabdev:QFN-12-1EP_2x2mm_P0.5mm_EP0.76x0.76mm (layer F.Cu) (tedit 5F53B4D4)
  (descr "QFN, 12 Pin, generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
  (tags "QFN DFN_QFN")
  (attr smd)
  (fp_text reference REF** (at 0 -2.45) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value QFN-12-1EP_2x2mm_P0.5mm_EP0.76x0.76mm (at 0 2.45) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 -4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -1) (end -1 0) (layer F.Fab) (width 0.15))
  (fp_line (start -1 0) (end -1 1) (layer F.Fab) (width 0.15))
  (fp_line (start -1 1) (end 1 1) (layer F.Fab) (width 0.15))
  (fp_line (start 1 1) (end 1 -1) (layer F.Fab) (width 0.15))
  (fp_line (start 1 -1) (end 0 -1) (layer F.Fab) (width 0.15))
  (fp_line (start 1 -1.15) (end 1.15 -1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.15 -1.15) (end 1.15 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 1 1.15) (end 1.15 1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.15 1.15) (end 1.15 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 1.15) (end -1.15 1.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.15 1.15) (end -1.15 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.45 -1.45) (end 1.45 -1.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.45 -1.45) (end 1.45 1.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.45 1.45) (end -1.45 1.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.45 1.45) (end -1.45 -1.45) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -1.5 -1.5) (end -1.35 -1.5) (layer F.SilkS) (width 0.3))
  (pad 1 smd rect (at -0.93 -0.5 90) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.93 0 90) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.93 0.5 90) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.5 0.93) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 0.93) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.5 0.93) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.93 0.5 90) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.93 0 90) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.93 -0.5 90) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.5 -0.93) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 -0.93) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -0.5 -0.93) (size 0.2 0.44) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -0.285 -0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at -0.285 -0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at -0.285 0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at -0.285 0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at -0.095 -0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at -0.095 -0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at -0.095 0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at -0.095 0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.095 -0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.095 -0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.095 0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.095 0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.285 -0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.285 -0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.285 0.095) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (pad 13 smd rect (at 0.285 0.285) (size 0.19 0.19) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.75))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-12-1EP_3x3mm_P0.5mm_EP1.65x1.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.67 0.67 0.67))
    (rotate (xyz 0 0 0))
  )
)
