(module Elabdev:Johanson_0868AT43A0020E_Down (layer F.Cu) (tedit 5F57B53B)
  (descr "868MHz Chip RF Antenna -1dBi Solder Surface Mount")
  (tags "antenna lora subghz subgigaherz")
  (attr smd)
  (fp_text reference ANT** (at 3 -3 unlocked) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Johanson_0868AT43A0020E (at 0 8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2 -1) (end 2 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 1) (end 2 1) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -0.8 0.3) (xy -2 0.3) (xy -2 -0.3) (xy -0.8 -0.3)) (layer F.SilkS) (width 0.1))
  (fp_line (start 4.8 -1.7) (end 4.8 6.8) (layer F.Fab) (width 0.12))
  (fp_line (start 4.8 6.8) (end -6.8 6.8) (layer F.Fab) (width 0.12))
  (fp_line (start -6.8 6.8) (end -6.8 -1.7) (layer F.Fab) (width 0.12))
  (fp_line (start -6.8 -1.7) (end 4.8 -1.7) (layer F.Fab) (width 0.12))
  (pad 1 smd rect (at -3.5 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.5 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -5 0) (size 2 1.2) (layers F.Cu))
  (pad 2 smd rect (at 3.75 3.45) (size 0.5 5.1) (layers F.Cu))
  (pad 2 smd rect (at 0.45 5.75) (size 7.1 0.5) (layers F.Cu))
  (pad 2 smd rect (at -2.85 4.5) (size 0.5 3) (layers F.Cu))
  (pad 2 smd rect (at -0.55 3.25) (size 5.1 0.5) (layers F.Cu))
)
