(module Elabdev:Oscillator_SMD_Taitien_TY-4Pin_2.5x2.0mm (layer F.Cu) (tedit 5F5382C7)
  (descr "SMD Crystal Oscillator Taitien TY (https://www.taitien.com/ti-products/standard-tcxo-series-ty-type/)")
  (tags "SMD SMT crystal oscillator")
  (attr smd)
  (fp_text reference REF** (at 0 -2.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Oscillator_SMD_Taitien_TY-4Pin_2.5x2.0mm (at 0 2.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.5 0.5) (thickness 0.08)))
  )
  (fp_line (start -1.25 -1) (end -1.25 1) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 1) (end 1.25 1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.25 1) (end 1.25 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.25 -1) (end -1.25 -1) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 0) (end -0.25 1) (layer F.Fab) (width 0.1))
  (fp_line (start -1.6 -1.3) (end -1.6 1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.6 1.3) (end 1.6 1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.7 -1.4) (end -1.7 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7 1.4) (end 1.7 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.7 1.4) (end 1.7 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.7 -1.4) (end -1.7 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_poly (pts (xy -0.8 1.3) (xy -1.6 1.3) (xy -1.6 0.5)) (layer F.SilkS) (width 0.1))
  (fp_circle (center -2.1 1.8) (end -1.95 1.8) (layer F.SilkS) (width 0.3))
  (pad 1 smd rect (at -0.85 0.65) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.85 0.65) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.85 -0.65) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.85 -0.65) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_SeikoEpson_SG210-4Pin_2.5x2.0mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
