EESchema-DOCLIB  Version 2.0
#
$CMP ATECC608A
D Elliptic Curve Crypto Authenticator
K Cryptography Authentication ECDSA FIPS186-3 ECDH FIPSSP800-56A I2C
F https://www.microchip.com/wwwproducts/ATECC608A/
$ENDCMP
#
$CMP ATSAMR34
D SAM R34/R35 Low Power LoRa Sub-GHz System-in-Package (SiP), Cortex-M0+ core, 256kB Flash, 40 KB RAM, 6x6mm TFBGA-64
K Atmel UHF Transceiver Microcontroller
F https://ww1.microchip.com/downloads/en/DeviceDoc/SAMR34-R35-Low-Power-LoRa-Sub-GHz-SiP-Data-Sheet-DS70005356B.pdf
$ENDCMP
#
$CMP BGS12SN6
D Infineon MOS SPDT absorbative switch, DC-6GHz, 40dB isolation at 868MHz, TSNP-6-2
K RF SPDT switch MOS absorbative
F https://www.infineon.com/dgdl/Infineon-BGS12SN6-DS-v02_03-EN.pdf
$ENDCMP
#
$CMP Logofirm
D Firma Logo
K Logo
F ~
$ENDCMP
#
$CMP MASW007935
D Macom GaAs RF SPDT absorbative switch, DC-3GHz, 1.1/22dB loss/isolation, SOT-26 (SOT-23-6)
K RF SPDT switch GaAs absorbative
F https://cdn.macom.com/datasheets/MASW-007935.pdf
$ENDCMP
#
$CMP SKY13373
D SP3T DC-6.0GHz switch, 30dB isolation at 2.5GHz, QFN-12
K RF SP3T switch CMOS
F http://www.skyworksinc.com/uploads/documents/SKY13373_460LF_201264N.pdf
$ENDCMP
#
$CMP STM32WLE5CCU6
D LPWAN Arm Cortex-M4 MCUs, LoRa, (G)FSK, (G)MSK, BPSK, 64/128/256KB Flash, 64KB SRAM, 7x7mm UFQFPN-48
K STM32 UHF Transceiver Microcontroller
F https://www.st.com/resource/datasheet/stm32wle5jc.pdf
$ENDCMP
#
$CMP Soldfeld
D Solder Area
K sf solder feld
$ENDCMP
#
$CMP TPS73533DRV
D 3.3V 500mA, Low Quiescent Current, Low Noise, High PSRR, Low-Dropout Linear Regulator, WSON-6
K ldo voltage regulator 500mA
F https://www.ti.com/lit/ds/symlink/tps735.pdf
$ENDCMP
#
$CMP TYETBCSANF
D 32MHz TCXO Clipped Sine Wave Oscillator
K Crystal Clock Oscillator
F http://www.taitien.com/wp-content/uploads/2015/12/XO-0081_TY.pdf
$ENDCMP
#
$CMP CMM-2718AB-383161
D MEMS Omnidirectional Digital Microphone, HLGA-3
K MEMS Microphone
F https://www.cui.com/product/resource/cmm-2718ab-383161-tr.pdf
$ENDCMP
#
$CMP ALSPT19
D Ambient Light Sensor, Phototransistor
K phototransistor ambient light sensor
F https://www.everlight.com/file/ProductFile/201407061531031645.pdf
$ENDCMP
#
$CMP USBCHole
D USB Type C Hole
K usb hole
$ENDCMP
#
$CMP Conn_ST_STDC14
D ST Debug Connector, standard ARM Cortex-M SWD and JTAG interface plus UART
K ST STM32 Cortex Debug Connector ARM SWD JTAG
F https://www.st.com/content/ccc/resource/technical/document/user_manual/group1/99/49/91/b6/b2/3a/46/e5/DM00526767/files/DM00526767.pdf/jcr:content/translations/en.DM00526767.pdf
$ENDCMP
#
$CMP ESD9B3.3ST5G
D ESD protection diode, 3.3Vrwm, SOD-923
K diode TVS ESD
F https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF
$ENDCMP
#
#End Doc Library
