(export (version D)
  (design
    (source dscomm.sch)
    (date "Mi 21 Okt 2020 18:45:11 CEST")
    (tool "Eeschema 5.1.5+dfsg1-2build2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source dscomm.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 2) (name /Sheet601C3EDD/) (tstamps /601C3EDE/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source feat-mchip.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 3) (name /Sheet5F84A570/) (tstamps /5F84A571/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source rfsw-stmicro.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 4) (name /Sheet60040980/) (tstamps /60040981/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source conn-mchip.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 5) (name /Sheet5F5C0727/) (tstamps /5F5C0728/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source rfsw-mchip.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 6) (name /Sheet5F53D5B4/) (tstamps /5F53D5B5/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source ctrl-mchip.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 7) (name /Sheet60040B89/) (tstamps /60040B8A/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source conn-stmicro.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 8) (name /Sheet60040A67/) (tstamps /60040A68/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source pwr-stmicro.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing"))))
    (sheet (number 9) (name /Sheet5F53D686/) (tstamps /5F53D687/)
      (title_block
        (title "Democratic Sendcomm")
        (company "Europalab Devices")
        (rev 0.8.5)
        (date 2020-10-20)
        (source ctrl-stmicro.sch)
        (comment (number 1) (value "Copyright © 2020, Europalab Devices"))
        (comment (number 2) (value "Fulfilling requirements of 20200210"))
        (comment (number 3) (value "Pending quality assurance testing"))
        (comment (number 4) (value "Release revision for manufacturing")))))
  (components
    (comp (ref FID1)
      (value Fiducial)
      (footprint Fiducial:Fiducial_0.5mm_Mask1.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4C4F46))
    (comp (ref FID2)
      (value Fiducial)
      (footprint Fiducial:Fiducial_0.5mm_Mask1.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4C52FB))
    (comp (ref MH1)
      (value MountingHole)
      (footprint Elabdev:Standoff_Keyelco_M3_2488X)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4C592E))
    (comp (ref MH4)
      (value MountingHole)
      (footprint Elabdev:Standoff_Keyelco_M3_2488X)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4C5CD0))
    (comp (ref MH7)
      (value MountingHole)
      (footprint Elabdev:Standoff_Keyelco_M3_2488X)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4C5F8D))
    (comp (ref MH10)
      (value MountingHole)
      (footprint Elabdev:Standoff_Keyelco_M3_2488X)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4C6223))
    (comp (ref FID3)
      (value Fiducial)
      (footprint Fiducial:Fiducial_0.5mm_Mask1.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4EEDB8))
    (comp (ref FID4)
      (value Fiducial)
      (footprint Fiducial:Fiducial_0.5mm_Mask1.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4EF4FC))
    (comp (ref MH2)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F7400E8))
    (comp (ref MH5)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F740657))
    (comp (ref MH8)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F740711))
    (comp (ref MH11)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F7407CB))
    (comp (ref MH3)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F740885))
    (comp (ref MH6)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F740F1C))
    (comp (ref MH9)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F740FD6))
    (comp (ref MH12)
      (value MountingHole)
      (footprint MountingHole:MountingHole_2.7mm_M2.5)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F741090))
    (comp (ref TP1)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Keystone_5005-5009_Compact)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F741DFB))
    (comp (ref TP2)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Keystone_5005-5009_Compact)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F742446))
    (comp (ref TP3)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Keystone_5005-5009_Compact)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F745479))
    (comp (ref TP4)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Keystone_5005-5009_Compact)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F7458A3))
    (comp (ref LOGO1)
      (value Logofirm)
      (footprint Elabdev:Elablogoslk-Gfx)
      (datasheet ~)
      (libsource (lib Elabdev) (part Logofirm) (description "Firma Logo"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F9652D3))
    (comp (ref TP5)
      (value Probe)
      (footprint TestPoint:TestPoint_THTPad_D2.5mm_Drill1.2mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Probe) (description "test point (alternative probe-style design)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F97637F))
    (comp (ref TP6)
      (value Probe)
      (footprint TestPoint:TestPoint_THTPad_D2.5mm_Drill1.2mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint_Probe) (description "test point (alternative probe-style design)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F97786E))
    (comp (ref U8)
      (value ATECC608A)
      (footprint Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm)
      (datasheet https://www.microchip.com/wwwproducts/ATECC608A/)
      (libsource (lib Elabdev) (part ATECC608A) (description "Elliptic Curve Crypto Authenticator"))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 601DBF43))
    (comp (ref R15)
      (value 4K7)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 601DBF61))
    (comp (ref R14)
      (value 4K7)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 601DBF67))
    (comp (ref U7)
      (value CAT24C32)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet https://www.onsemi.com/pub/Collateral/CAT24C32-D.PDF)
      (libsource (lib Memory_EEPROM) (part CAT24C256) (description "256 kb CMOS Serial EEPROM, DIP-8/SOIC-8/TSSOP-8/DFN-8"))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F68A355))
    (comp (ref C41)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F68CC64))
    (comp (ref R11)
      (value 3K9)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F6983A1))
    (comp (ref R12)
      (value 3K9)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F698FB0))
    (comp (ref R13)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F6990E6))
    (comp (ref J7)
      (value Conn_01x02_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F69B305))
    (comp (ref U6)
      (value CAT24C32)
      (footprint Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm)
      (datasheet https://www.onsemi.com/pub/Collateral/CAT24C32-D.PDF)
      (libsource (lib Memory_EEPROM) (part CAT24C256) (description "256 kb CMOS Serial EEPROM, DIP-8/SOIC-8/TSSOP-8/DFN-8"))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F70A85A))
    (comp (ref U9)
      (value ATECC608A)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet https://www.microchip.com/wwwproducts/ATECC608A/)
      (libsource (lib Elabdev) (part ATECC608A) (description "Elliptic Curve Crypto Authenticator"))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F74CA64))
    (comp (ref C42)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet601C3EDD/) (tstamps /601C3EDE/))
      (tstamp 5F78EE57))
    (comp (ref U11)
      (value MASW007935)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet https://cdn.macom.com/datasheets/MASW-007935.pdf)
      (libsource (lib Elabdev) (part MASW007935) (description "Macom GaAs RF SPDT absorbative switch, DC-3GHz, 1.1/22dB loss/isolation, SOT-26 (SOT-23-6)"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F86275C))
    (comp (ref C46)
      (value 39pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8AB1DB))
    (comp (ref C47)
      (value 39pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8ABC2C))
    (comp (ref C45)
      (value 100pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8AD0D2))
    (comp (ref C44)
      (value 39pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8AF02D))
    (comp (ref U1)
      (value BGS12SN6)
      (footprint Elabdev:TSNP-6_0.7x1.1mm_P0.4mm)
      (datasheet https://www.infineon.com/dgdl/Infineon-BGS12SN6-DS-v02_03-EN.pdf)
      (libsource (lib Elabdev) (part BGS12SN6) (description "Infineon MOS SPDT absorbative switch, DC-6GHz, 40dB isolation at 868MHz, TSNP-6-2"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8B3B9D))
    (comp (ref C43)
      (value 100pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8C4134))
    (comp (ref C48)
      (value 1nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8C6C09))
    (comp (ref U10)
      (value MSWA-2-20)
      (footprint Package_SO:SOP-8_3.76x4.96mm_P1.27mm)
      (datasheet https://www.minicircuits.com/pdfs/MSWA-2-20+.pdf)
      (libsource (lib RF_Switch) (part MSWA-2-20) (description "SPDT DC-2.0GHz absorbative switch, 50 Ohm, SOP-8"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 5F8D4013))
    (comp (ref C54)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B4F238))
    (comp (ref C58)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B50234))
    (comp (ref L12)
      (value 0R)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B5130C))
    (comp (ref C50)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Placement) DNP))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B5E5E5))
    (comp (ref C55)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6ADAF))
    (comp (ref C59)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6ADB9))
    (comp (ref L13)
      (value 0R)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6ADC3))
    (comp (ref C51)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Placement) DNP))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6ADD7))
    (comp (ref J8)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6E11F))
    (comp (ref C53)
      (value 3,3pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6E13D))
    (comp (ref C57)
      (value 3,3pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6E147))
    (comp (ref L11)
      (value 8,7nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6E151))
    (comp (ref C49)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B6E165))
    (comp (ref AE8)
      (value Antenna_Shield)
      (footprint Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Shield) (description "Antenna with extra pin for shielding"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B7220E))
    (comp (ref AE10)
      (value Antenna_Chip)
      (footprint Elabdev:Johanson_0868AT43A0020E_Down)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Chip) (description "Ceramic chip antenna with pin for PCB trace"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B75D15))
    (comp (ref C56)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B7A97E))
    (comp (ref C60)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B7A988))
    (comp (ref L14)
      (value 0R)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B7A992))
    (comp (ref C52)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Placement) DNP))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B7A9A7))
    (comp (ref AE9)
      (value Antenna)
      (footprint RF_Antenna:Texas_SWRA416_868MHz_915MHz)
      (datasheet ~)
      (libsource (lib Device) (part Antenna) (description Antenna))
      (sheetpath (names /Sheet5F84A570/) (tstamps /5F84A571/))
      (tstamp 60B7E7BB))
    (comp (ref J5)
      (value Conn_01x06_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06_Male) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6006812D))
    (comp (ref R9)
      (value 100K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 600B7E79))
    (comp (ref J4)
      (value Conn_ARM_JTAG_SWD_10)
      (footprint Connector:Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical)
      (datasheet http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf)
      (libsource (lib Connector) (part Conn_ARM_JTAG_SWD_10) (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 600B7E84))
    (comp (ref J3)
      (value RPIHAT-40W)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical)
      (datasheet https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf)
      (libsource (lib Connector) (part Raspberry_Pi_2_3) (description "expansion header for Raspberry Pi 2 & 3"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 5F6A7FD9))
    (comp (ref JP2)
      (value Jumper_NO_Small)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 5F6EEE9D))
    (comp (ref JP3)
      (value Jumper_NO_Small)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 5F6F4E2A))
    (comp (ref R8)
      (value 2K4)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6005D79D))
    (comp (ref R7)
      (value 2K4)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6005D791))
    (comp (ref R6)
      (value 47K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6005D77E))
    (comp (ref R5)
      (value 47K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6005D774))
    (comp (ref U5)
      (value NUP2202)
      (footprint Package_TO_SOT_SMD:SOT-363_SC-70-6)
      (datasheet http://www.onsemi.ru.com/pub_link/Collateral/NUP2202W1-D.PDF)
      (libsource (lib Power_Protection) (part NUP2202) (description "Transient voltage suppressor designed to protect high speed data lines from ESD, EFT, and lightning"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6005D760))
    (comp (ref C40)
      (value 4,7nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6005D746))
    (comp (ref R10)
      (value 1M)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 6005D740))
    (comp (ref J2)
      (value USB_C_Receptacle_USB2.0)
      (footprint Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12)
      (datasheet https://www.usb.org/sites/default/files/documents/usb_type-c.zip)
      (libsource (lib Connector) (part USB_C_Receptacle_USB2.0) (description "USB 2.0-only Type-C Receptacle connector"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 5F8FC344))
    (comp (ref J6)
      (value Conn_02x04_Top_Bottom)
      (footprint Elabdev:Millmax_Pogopin_2x4_P2.54mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x04_Top_Bottom) (description "Generic connector, double row, 02x04, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 5F9DDFF1))
    (comp (ref SF1)
      (value Soldfeld)
      (footprint Elabdev:SolderlittleArea_8)
      (libsource (lib Elabdev) (part Soldfeld) (description "Solder Area"))
      (sheetpath (names /Sheet60040980/) (tstamps /60040981/))
      (tstamp 5FA04057))
    (comp (ref U4)
      (value SKY13373)
      (footprint Elabdev:QFN-12-1EP_2x2mm_P0.5mm_EP0.76x0.76mm)
      (datasheet http://www.skyworksinc.com/uploads/documents/SKY13373_460LF_201264N.pdf)
      (libsource (lib Elabdev) (part SKY13373) (description "SP3T DC-6.0GHz switch, 30dB isolation at 2.5GHz, QFN-12"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6D5B))
    (comp (ref AE2)
      (value Antenna_Shield)
      (footprint Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Shield) (description "Antenna with extra pin for shielding"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6D7C))
    (comp (ref C22)
      (value 1nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6D8A))
    (comp (ref C29)
      (value 47pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6D9A))
    (comp (ref C30)
      (value 27pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DA0))
    (comp (ref L6)
      (value 10nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DA6))
    (comp (ref L8)
      (value 10nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DB8))
    (comp (ref L9)
      (value 10nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DC1))
    (comp (ref L10)
      (value 11nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DC7))
    (comp (ref C35)
      (value 22pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DCD))
    (comp (ref C33)
      (value DNP)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DD9))
    (comp (ref C34)
      (value DNP)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DDF))
    (comp (ref C36)
      (value 3,3pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DF1))
    (comp (ref C37)
      (value 5,6pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6DF9))
    (comp (ref C38)
      (value 8,2pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E01))
    (comp (ref C39)
      (value 3,9pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E09))
    (comp (ref L2)
      (value 10nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E20))
    (comp (ref L3)
      (value 10nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E27))
    (comp (ref L4)
      (value 2,2nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E2D))
    (comp (ref C24)
      (value 18pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E33))
    (comp (ref C23)
      (value DNP)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E3E))
    (comp (ref C25)
      (value 3,3pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E48))
    (comp (ref C26)
      (value 5,6pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E50))
    (comp (ref C27)
      (value 3,3pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E57))
    (comp (ref C28)
      (value 3,9pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E5F))
    (comp (ref L5)
      (value 33nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E7A))
    (comp (ref L7)
      (value 33nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E84))
    (comp (ref C32)
      (value DNP)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E8E))
    (comp (ref C31)
      (value 4,7nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F5D6E94))
    (comp (ref AE4)
      (value Antenna_Shield)
      (footprint Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Shield) (description "Antenna with extra pin for shielding"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 6000659E))
    (comp (ref AE6)
      (value Antenna_Shield)
      (footprint Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Shield) (description "Antenna with extra pin for shielding"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 60006A31))
    (comp (ref AE7)
      (value Antenna_Shield)
      (footprint Connector_Coaxial:SMA_Amphenol_132289_EdgeMount)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Shield) (description "Antenna with extra pin for shielding"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 6000721D))
    (comp (ref AE1)
      (value Antenna)
      (footprint RF_Antenna:Texas_SWRA416_868MHz_915MHz)
      (datasheet ~)
      (libsource (lib Device) (part Antenna) (description Antenna))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 60008187))
    (comp (ref AE5)
      (value Antenna_Chip)
      (footprint Elabdev:Johanson_0868AT43A0020E_Down)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Chip) (description "Ceramic chip antenna with pin for PCB trace"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 60008781))
    (comp (ref AE3)
      (value Antenna_Chip)
      (footprint Elabdev:Linx_ANT-868-SP_38x98mm)
      (datasheet ~)
      (libsource (lib Device) (part Antenna_Chip) (description "Ceramic chip antenna with pin for PCB trace"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 6045549B))
    (comp (ref JP4)
      (value SolderBridge)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F989558))
    (comp (ref JP6)
      (value SolderJump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F98A4D6))
    (comp (ref JP5)
      (value SolderJump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F98B50E))
    (comp (ref JP8)
      (value SolderJump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F98BA4E))
    (comp (ref JP7)
      (value SolderJump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F98BF79))
    (comp (ref JP9)
      (value SolderJump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F98C3E5))
    (comp (ref JP10)
      (value SolderJump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F5C0727/) (tstamps /5F5C0728/))
      (tstamp 5F98C778))
    (comp (ref C18)
      (value 10pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F60A467))
    (comp (ref Y1)
      (value Crystal)
      (footprint Crystal:Crystal_SMD_MicroCrystal_CM9V-T1A-2Pin_1.6x1.0mm)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F606FD8))
    (comp (ref XC1)
      (value TYETBCSANF)
      (footprint Elabdev:Oscillator_SMD_Taitien_TY-4Pin_2.5x2.0mm)
      (datasheet http://www.taitien.com/wp-content/uploads/2015/12/XO-0081_TY.pdf)
      (libsource (lib Elabdev) (part TYETBCSANF) (description "32MHz TCXO Clipped Sine Wave Oscillator"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F60E7DB))
    (comp (ref C21)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F611282))
    (comp (ref C9)
      (value 10uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F6159D4))
    (comp (ref L1)
      (value LQH3NPN100MJRL)
      (footprint Inductor_SMD:L_Vishay_IHLP-1212)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F643B51))
    (comp (ref C17)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F644AA5))
    (comp (ref C10)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F6C3BDA))
    (comp (ref C11)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F6C40B2))
    (comp (ref C12)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F6EF828))
    (comp (ref C15)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F6F34AF))
    (comp (ref C14)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F700C24))
    (comp (ref C13)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F715342))
    (comp (ref C4)
      (value 4,7pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F7E81D0))
    (comp (ref C2)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F80DBCB))
    (comp (ref C1)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F81B8EA))
    (comp (ref C16)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F824E62))
    (comp (ref SW1)
      (value SW_SPST)
      (footprint Button_Switch_SMD:SW_SPST_PTS810)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPST) (description "Single Pole Single Throw (SPST) switch"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F8E32A8))
    (comp (ref R3)
      (value 39)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F8FAD6F))
    (comp (ref C20)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F9C9E31))
    (comp (ref J1)
      (value Conn_01x03_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x03_Male) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FA30206))
    (comp (ref BT1)
      (value Battery_Cell)
      (footprint Battery:BatteryHolder_Keystone_3002_1x2032)
      (datasheet ~)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FA3E7CA))
    (comp (ref SW2)
      (value SW_SPST)
      (footprint Button_Switch_SMD:SW_SPST_PTS810)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPST) (description "Single Pole Single Throw (SPST) switch"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FA530DE))
    (comp (ref R4)
      (value 39)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FA55193))
    (comp (ref U2)
      (value TPS73533DRV)
      (footprint Package_SON:Texas_PWSON-N6)
      (datasheet https://www.ti.com/lit/ds/symlink/tps735.pdf)
      (libsource (lib Elabdev) (part TPS73533DRV) (description "3.3V 500mA, Low Quiescent Current, Low Noise, High PSRR, Low-Dropout Linear Regulator, WSON-6"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FA8FBF4))
    (comp (ref C8)
      (value 10nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FAA65B5))
    (comp (ref C7)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FAA6ED2))
    (comp (ref C6)
      (value 4,7uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FAF7D0B))
    (comp (ref C5)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FAFF8F3))
    (comp (ref JP1)
      (value Jumper_2_Bridged)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Jumper) (part Jumper_2_Bridged) (description "Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FB3D721))
    (comp (ref D1)
      (value GREEN)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FB63E55))
    (comp (ref D2)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FB6459F))
    (comp (ref R1)
      (value 330)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FB8F84E))
    (comp (ref R2)
      (value 330)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5FB8FDC5))
    (comp (ref C3)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F7EC846))
    (comp (ref FB1)
      (value BLM15AG121SN1D)
      (footprint Inductor_SMD:L_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part Ferrite_Bead) (description "Ferrite bead"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F613B5F))
    (comp (ref U3)
      (value ATSAMR34)
      (footprint Elabdev:TFBGA-64_8x8_6.0x6.0mm_P0.65mm)
      (datasheet https://ww1.microchip.com/downloads/en/DeviceDoc/SAMR34-R35-Low-Power-LoRa-Sub-GHz-SiP-Data-Sheet-DS70005356B.pdf)
      (libsource (lib Elabdev) (part ATSAMR34) (description "SAM R34/R35 Low Power LoRa Sub-GHz System-in-Package (SiP), Cortex-M0+ core, 256kB Flash, 40 KB RAM, 6x6mm TFBGA-64"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 6052EF69))
    (comp (ref C19)
      (value 10pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D5B4/) (tstamps /5F53D5B5/))
      (tstamp 5F609CF5))
    (comp (ref U13)
      (value CAT24C32)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet https://www.onsemi.com/pub/Collateral/CAT24C32-D.PDF)
      (libsource (lib Memory_EEPROM) (part CAT24C256) (description "256 kb CMOS Serial EEPROM, DIP-8/SOIC-8/TSSOP-8/DFN-8"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BCE932))
    (comp (ref C61)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BCE956))
    (comp (ref R16)
      (value 3K9)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BCE95C))
    (comp (ref R17)
      (value 3K9)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BCE962))
    (comp (ref R18)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BCE968))
    (comp (ref J15)
      (value Conn_01x02_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BCE978))
    (comp (ref U12)
      (value CAT24C32)
      (footprint Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm)
      (datasheet https://www.onsemi.com/pub/Collateral/CAT24C32-D.PDF)
      (libsource (lib Memory_EEPROM) (part CAT24C256) (description "256 kb CMOS Serial EEPROM, DIP-8/SOIC-8/TSSOP-8/DFN-8"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BCE989))
    (comp (ref J11)
      (value RPIHAT-40W)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical)
      (datasheet https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf)
      (libsource (lib Connector) (part Raspberry_Pi_2_3) (description "expansion header for Raspberry Pi 2 & 3"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BE538F))
    (comp (ref JP11)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BE53DB))
    (comp (ref JP12)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60BE53E1))
    (comp (ref JP13)
      (value Solderjump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60C4BB6A))
    (comp (ref JP14)
      (value Solderjump)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 60C4C66F))
    (comp (ref J13)
      (value CN_PMOD_GPIO)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x06) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5F94ABFC))
    (comp (ref J14)
      (value CN_Mikroclick)
      (footprint Elabdev:Mikrobus_Host_Conn)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise) (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5F94CB08))
    (comp (ref J9)
      (value CN_UART)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x06) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5F9F77C0))
    (comp (ref JP15)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FBC816A))
    (comp (ref JP16)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FBD3983))
    (comp (ref JP17)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FBD59C0))
    (comp (ref JP18)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FBD59CB))
    (comp (ref J12)
      (value CN_PMOD_I2C)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x06_Odd_Even) (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FBA8BB7))
    (comp (ref JP19)
      (value Jmp-RST)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FC45157))
    (comp (ref J16)
      (value CN_Test)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FC50DE9))
    (comp (ref JP20)
      (value Test-A)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FC5EEF8))
    (comp (ref JP21)
      (value Test-B)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NO_Small) (description "Jumper, normally open, small symbol"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FC61B86))
    (comp (ref J10)
      (value Conn_02x04_Top_Bottom)
      (footprint Elabdev:Millmax_Pogopin_2x4_P2.54mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x04_Top_Bottom) (description "Generic connector, double row, 02x04, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FC80C9D))
    (comp (ref SF2)
      (value Soldfeld)
      (footprint Elabdev:SolderlittleArea_8)
      (libsource (lib Elabdev) (part Soldfeld) (description "Solder Area"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5FC80CAC))
    (comp (ref J19)
      (value CN_Grove)
      (footprint Connector_JST:JST_PH_B4B-PH-SM4-TB_1x04-1MP_P2.00mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Sheet60040B89/) (tstamps /60040B8A/))
      (tstamp 5F97367E))
    (comp (ref C72)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD68E))
    (comp (ref C73)
      (value 4,7uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD694))
    (comp (ref BT2)
      (value Battery_Cell)
      (footprint Battery:BatteryHolder_Keystone_3002_1x2032)
      (datasheet ~)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD69E))
    (comp (ref C69)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD6A7))
    (comp (ref C62)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD6AF))
    (comp (ref C64)
      (value 4,7uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD6B5))
    (comp (ref C70)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD6C1))
    (comp (ref C71)
      (value 4,7uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD6CB))
    (comp (ref C68)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD6DB))
    (comp (ref C67)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD6F6))
    (comp (ref L16)
      (value 15uH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD707))
    (comp (ref C66)
      (value 0,47uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD70D))
    (comp (ref R19)
      (value 0)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD713))
    (comp (ref C65)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD71E))
    (comp (ref C63)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD732))
    (comp (ref L15)
      (value 600)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet60040A67/) (tstamps /60040A68/))
      (tstamp 601CD751))
    (comp (ref D3)
      (value LED)
      (footprint Diode_SMD:D_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Colour) BLUE))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F91265F))
    (comp (ref R28)
      (value 120)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F913444))
    (comp (ref D4)
      (value LED)
      (footprint Diode_SMD:D_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Colour) GREEN))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F91486B))
    (comp (ref R29)
      (value 270)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F914875))
    (comp (ref D5)
      (value LED)
      (footprint Diode_SMD:D_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Colour) RED))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F915791))
    (comp (ref R30)
      (value 360)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F91579B))
    (comp (ref SW3)
      (value SPST)
      (footprint Button_Switch_SMD:SW_SPST_PTS810)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPST) (description "Single Pole Single Throw (SPST) switch"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F91A2D7))
    (comp (ref R25)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F91DE69))
    (comp (ref R26)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F91F462))
    (comp (ref SW4)
      (value SPST)
      (footprint Button_Switch_SMD:SW_SPST_PTS810)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPST) (description "Single Pole Single Throw (SPST) switch"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F91F456))
    (comp (ref R27)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F92C857))
    (comp (ref SW5)
      (value SPST)
      (footprint Button_Switch_SMD:SW_SPST_PTS810)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPST) (description "Single Pole Single Throw (SPST) switch"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F92C862))
    (comp (ref C78)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F9329C5))
    (comp (ref D6)
      (value SP0503BAHT)
      (footprint Package_TO_SOT_SMD:SOT-143)
      (datasheet http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf)
      (libsource (lib Power_Protection) (part SP0503BAHT) (description "TVS Diode Array, 5.5V Standoff, 3 Channels, SOT-143 package"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F937FCA))
    (comp (ref C80)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F93A1B6))
    (comp (ref C79)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F938DC1))
    (comp (ref JP24)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, normally closed"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FB9645E))
    (comp (ref R31)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FB96CB5))
    (comp (ref C91)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FB9DA34))
    (comp (ref D7)
      (value ESD9B3.3ST5G)
      (footprint Elabdev:D_SOD-923)
      (datasheet https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF)
      (libsource (lib Elabdev) (part ESD9B3.3ST5G) (description "ESD protection diode, 3.3Vrwm, SOD-923"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FBA9E71))
    (comp (ref SW6)
      (value SPST)
      (footprint Button_Switch_SMD:SW_SPST_PTS810)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPST) (description "Single Pole Single Throw (SPST) switch"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FB9D233))
    (comp (ref J18)
      (value CN_STDC14)
      (footprint Connector_PinSocket_1.27mm:PinSocket_2x07_P1.27mm_Vertical_SMD)
      (datasheet https://www.st.com/content/ccc/resource/technical/document/user_manual/group1/99/49/91/b6/b2/3a/46/e5/DM00526767/files/DM00526767.pdf/jcr:content/translations/en.DM00526767.pdf)
      (libsource (lib Elabdev) (part Conn_ST_STDC14) (description "ST Debug Connector, standard ARM Cortex-M SWD and JTAG interface plus UART"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FC1F936))
    (comp (ref J17)
      (value CN_JTAGSWD)
      (footprint Connector:Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical)
      (datasheet http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf)
      (libsource (lib Connector) (part Conn_ARM_JTAG_SWD_10) (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FC20BA3))
    (comp (ref R38)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FD01677))
    (comp (ref R33)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FD1B023))
    (comp (ref R36)
      (value 47)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FD629DD))
    (comp (ref R37)
      (value 47)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FD63992))
    (comp (ref R20)
      (value 47)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FDE338F))
    (comp (ref R21)
      (value 47)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FE0144B))
    (comp (ref R22)
      (value 47)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FE014D9))
    (comp (ref R23)
      (value 47)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FE01562))
    (comp (ref R24)
      (value 47)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FE015EB))
    (comp (ref U14)
      (value STM32WLE5CCU6)
      (footprint Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm)
      (datasheet https://www.st.com/resource/datasheet/stm32wle5jc.pdf)
      (libsource (lib Elabdev) (part STM32WLE5CCU6) (description "LPWAN Arm Cortex-M4 MCUs, LoRa, (G)FSK, (G)MSK, BPSK, 64/128/256KB Flash, 64KB SRAM, 7x7mm UFQFPN-48"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FF9B835))
    (comp (ref TH1)
      (value Thermistor)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part Thermistor) (description "Temperature dependent resistor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 600C68EA))
    (comp (ref Y3)
      (value NX2012SA)
      (footprint Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm)
      (datasheet ~)
      (fields
        (field (name Speed) 32KHz))
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 6032E22E))
    (comp (ref Y2)
      (value NX2016SA)
      (footprint Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm)
      (datasheet ~)
      (fields
        (field (name Speed) 32MHz))
      (libsource (lib Device) (part Crystal_GND24) (description "Four pin crystal, GND on pins 2 and 4"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 6032E62A))
    (comp (ref C76)
      (value 7pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 603459B1))
    (comp (ref C77)
      (value 7pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 6034D3D2))
    (comp (ref JP25)
      (value SJMP)
      (footprint Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_3_Bridged12) (description "3-pole Solder Jumper, pins 1+2 closed/bridged"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 604ADC57))
    (comp (ref C81)
      (value 47nF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 60506788))
    (comp (ref C82)
      (value 68pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 605071CB))
    (comp (ref C74)
      (value 6,8pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 605597F3))
    (comp (ref C75)
      (value 6,8pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 605634E0))
    (comp (ref C83)
      (value 6,8pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 606109A8))
    (comp (ref L18)
      (value 47nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 604A4410))
    (comp (ref L17)
      (value 3,6nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 604E055B))
    (comp (ref C85)
      (value 3,9pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 6061E220))
    (comp (ref L20)
      (value 3,3nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 605D7DF1))
    (comp (ref L21)
      (value 6,8nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 60665100))
    (comp (ref C89)
      (value 2,7pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 60671D3B))
    (comp (ref C87)
      (value 33pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 605EDB09))
    (comp (ref C86)
      (value 2,7pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 60713402))
    (comp (ref C84)
      (value 2,4pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 6064C7F1))
    (comp (ref L19)
      (value 11nH)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 6072062D))
    (comp (ref C88)
      (value 3,6pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 60780CD1))
    (comp (ref C90)
      (value 1pF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Placement) DNP))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 607B3F58))
    (comp (ref Q1)
      (value ALSPT19)
      (footprint Elabdev:ALS_TR8_SMT)
      (datasheet https://www.everlight.com/file/ProductFile/201407061531031645.pdf)
      (libsource (lib Elabdev) (part ALSPT19) (description "Ambient Light Sensor, Phototransistor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 608E48BC))
    (comp (ref R34)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 608E51DE))
    (comp (ref JP22)
      (value SolderJumper)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 60C15DFA))
    (comp (ref JP23)
      (value SolderJumper)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 60C3D9E5))
    (comp (ref R32)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F96FE4B))
    (comp (ref R35)
      (value 100K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FC92B56))
    (comp (ref MIC1)
      (value CMM-2718AB-383161)
      (footprint Elabdev:CMM-2718AB-383161)
      (datasheet https://www.cui.com/product/resource/cmm-2718ab-383161-tr.pdf)
      (libsource (lib Elabdev) (part CMM-2718AB-383161) (description "MEMS Omnidirectional Digital Microphone, HLGA-3"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F9D1A0D))
    (comp (ref C93)
      (value 10uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name Placement) Maybe-DNP))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5F9EFBBD))
    (comp (ref C92)
      (value 0,1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5F53D686/) (tstamps /5F53D687/))
      (tstamp 5FA0A493)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x03_Male)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector) (part Conn_01x06_Male)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector) (part Conn_ARM_JTAG_SWD_10)
      (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface")
      (docs http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf)
      (footprints
        (fp PinHeader?2x05?P1.27mm*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_ARM_JTAG_SWD_10))
      (pins
        (pin (num 1) (name VTref) (type power_in))
        (pin (num 2) (name SWDIO/TMS) (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name SWDCLK/TCK) (type output))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name SWO/TDO) (type input))
        (pin (num 7) (name KEY) (type NotConnected))
        (pin (num 8) (name NC/TDI) (type output))
        (pin (num 9) (name GNDDetect) (type passive))
        (pin (num 10) (name ~RESET~) (type openCol))))
    (libpart (lib Connector) (part Conn_Coaxial)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (docs " ~")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib Connector) (part Raspberry_Pi_2_3)
      (description "expansion header for Raspberry Pi 2 & 3")
      (docs https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf)
      (footprints
        (fp PinHeader*2x20*P2.54mm*Vertical*)
        (fp PinSocket*2x20*P2.54mm*Vertical*))
      (fields
        (field (name Reference) J)
        (field (name Value) Raspberry_Pi_2_3))
      (pins
        (pin (num 1) (name 3V3) (type power_in))
        (pin (num 2) (name 5V) (type power_in))
        (pin (num 3) (name SDA/GPIO2) (type BiDi))
        (pin (num 4) (name 5V) (type power_in))
        (pin (num 5) (name SCL/GPIO3) (type BiDi))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name GCLK0/GPIO4) (type BiDi))
        (pin (num 8) (name GPIO14/TXD) (type BiDi))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name GPIO15/RXD) (type BiDi))
        (pin (num 11) (name GPIO17) (type BiDi))
        (pin (num 12) (name GPIO18/PWM0) (type BiDi))
        (pin (num 13) (name GPIO27) (type BiDi))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name GPIO22) (type BiDi))
        (pin (num 16) (name GPIO23) (type BiDi))
        (pin (num 17) (name 3V3) (type power_in))
        (pin (num 18) (name GPIO24) (type BiDi))
        (pin (num 19) (name MOSI0/GPIO10) (type BiDi))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name MISO0/GPIO9) (type BiDi))
        (pin (num 22) (name GPIO25) (type BiDi))
        (pin (num 23) (name SCLK0/GPIO11) (type BiDi))
        (pin (num 24) (name ~CE0~/GPIO8) (type BiDi))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name ~CE1~/GPIO7) (type BiDi))
        (pin (num 27) (name ID_SD/GPIO0) (type BiDi))
        (pin (num 28) (name ID_SC/GPIO1) (type BiDi))
        (pin (num 29) (name GCLK1/GPIO5) (type BiDi))
        (pin (num 30) (name GND) (type power_in))
        (pin (num 31) (name GCLK2/GPIO6) (type BiDi))
        (pin (num 32) (name PWM0/GPIO12) (type BiDi))
        (pin (num 33) (name PWM1/GPIO13) (type BiDi))
        (pin (num 34) (name GND) (type power_in))
        (pin (num 35) (name GPIO19/MISO1) (type BiDi))
        (pin (num 36) (name GPIO16) (type BiDi))
        (pin (num 37) (name GPIO26) (type BiDi))
        (pin (num 38) (name GPIO20/MOSI1) (type BiDi))
        (pin (num 39) (name GND) (type power_in))
        (pin (num 40) (name GPIO21/SCLK1) (type BiDi))))
    (libpart (lib Connector) (part TestPoint)
      (description "test point")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Connector) (part TestPoint_Probe)
      (description "test point (alternative probe-style design)")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint_Probe))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Connector) (part USB_C_Receptacle_USB2.0)
      (description "USB 2.0-only Type-C Receptacle connector")
      (docs https://www.usb.org/sites/default/files/documents/usb_type-c.zip)
      (footprints
        (fp USB*C*Receptacle*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_C_Receptacle_USB2.0))
      (pins
        (pin (num A1) (name GND) (type power_in))
        (pin (num A4) (name VBUS) (type power_in))
        (pin (num A5) (name CC1) (type BiDi))
        (pin (num A6) (name D+) (type BiDi))
        (pin (num A7) (name D-) (type BiDi))
        (pin (num A8) (name SBU1) (type BiDi))
        (pin (num A9) (name VBUS) (type passive))
        (pin (num A12) (name GND) (type passive))
        (pin (num B1) (name GND) (type passive))
        (pin (num B4) (name VBUS) (type passive))
        (pin (num B5) (name CC2) (type BiDi))
        (pin (num B6) (name D+) (type BiDi))
        (pin (num B7) (name D-) (type BiDi))
        (pin (num B8) (name SBU2) (type BiDi))
        (pin (num B9) (name VBUS) (type passive))
        (pin (num B12) (name GND) (type passive))
        (pin (num S1) (name SHIELD) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x06)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x04_Top_Bottom)
      (description "Generic connector, double row, 02x04, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x04_Top_Bottom))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x06_Odd_Even)
      (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x06_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise)
      (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x08_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))))
    (libpart (lib Device) (part Antenna)
      (description Antenna)
      (docs ~)
      (fields
        (field (name Reference) AE)
        (field (name Value) Antenna))
      (pins
        (pin (num 1) (name A) (type input))))
    (libpart (lib Device) (part Antenna_Chip)
      (description "Ceramic chip antenna with pin for PCB trace")
      (docs ~)
      (fields
        (field (name Reference) AE)
        (field (name Value) Antenna_Chip))
      (pins
        (pin (num 1) (name FEED) (type input))
        (pin (num 2) (name PCB_Trace) (type passive))))
    (libpart (lib Device) (part Antenna_Shield)
      (description "Antenna with extra pin for shielding")
      (docs ~)
      (fields
        (field (name Reference) AE)
        (field (name Value) Antenna_Shield))
      (pins
        (pin (num 1) (name A) (type input))
        (pin (num 2) (name Shield) (type input))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal)
      (description "Two pin crystal")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part Crystal_GND24)
      (description "Four pin crystal, GND on pins 2 and 4")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND24))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead)
      (description "Ferrite bead")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Jumper)
      (description "Jumper, normally closed")
      (docs ~)
      (footprints
        (fp SolderJumper*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part Jumper_NO_Small)
      (description "Jumper, normally open, small symbol")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part L_Small)
      (description "Inductor, small symbol")
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Thermistor)
      (description "Temperature dependent resistor")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) TH)
        (field (name Value) Thermistor))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Elabdev) (part ALSPT19)
      (description "Ambient Light Sensor, Phototransistor")
      (docs https://www.everlight.com/file/ProductFile/201407061531031645.pdf)
      (footprints
        (fp ALS_TR8_*))
      (fields
        (field (name Reference) Q)
        (field (name Value) ALSPT19)
        (field (name Footprint) Elabdev:ALS_TR8_SMT))
      (pins
        (pin (num 1) (name C) (type power_in))
        (pin (num 2) (name E) (type output))))
    (libpart (lib Elabdev) (part ATECC608A)
      (aliases
        (alias ATECC608A-MAHDA-S)
        (alias ATECC608A-SSHDA-T)
        (alias ATECC508A-MAHDA-S)
        (alias ATECC508A-SSHDA-T))
      (description "Elliptic Curve Crypto Authenticator")
      (docs https://www.microchip.com/wwwproducts/ATECC608A/)
      (footprints
        (fp DFN-8-*2x3mm_Pitch0.5mm*)
        (fp SOIC-8*3.9x4.9mm_Pitch1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ATECC608A)
        (field (name Footprint) Housings_DFN_QFN:DFN-8-1EP_2x3mm_Pitch0.5mm)
        (field (name Datasheet) http://ww1.microchip.com/downloads/en/DeviceDoc/20005927A.pdf))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name NC) (type NotConnected))
        (pin (num 3) (name NC) (type NotConnected))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name SDA) (type BiDi))
        (pin (num 6) (name SCL) (type input))
        (pin (num 7) (name NC) (type NotConnected))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Elabdev) (part ATSAMR34)
      (description "SAM R34/R35 Low Power LoRa Sub-GHz System-in-Package (SiP), Cortex-M0+ core, 256kB Flash, 40 KB RAM, 6x6mm TFBGA-64")
      (docs https://ww1.microchip.com/downloads/en/DeviceDoc/SAMR34-R35-Low-Power-LoRa-Sub-GHz-SiP-Data-Sheet-DS70005356B.pdf)
      (footprints
        (fp TFBGA*8x8mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ATSAMR34)
        (field (name Footprint) Elabdev:TFBGA-64_8x8_6.0x6.0mm_P0.65mm)
        (field (name Datasheet) https://www.microchip.com/wwwproducts/ATSAMR34J18/))
      (pins
        (pin (num A1) (name RFI_HF) (type input))
        (pin (num A2) (name GND_RF) (type power_in))
        (pin (num A3) (name PA00) (type BiDi))
        (pin (num A4) (name PA01) (type BiDi))
        (pin (num A5) (name VDDCORE) (type power_in))
        (pin (num A6) (name VSW) (type power_in))
        (pin (num A7) (name VDDIN) (type power_in))
        (pin (num A8) (name VDDIO2) (type power_in))
        (pin (num B1) (name RFO_HF) (type output))
        (pin (num B2) (name GND_RF) (type power_in))
        (pin (num B3) (name GNDANA) (type power_in))
        (pin (num B4) (name PB02) (type BiDi))
        (pin (num B5) (name GND) (type power_in))
        (pin (num B6) (name RESET) (type input))
        (pin (num B7) (name GND) (type power_in))
        (pin (num B8) (name PA24) (type BiDi))
        (pin (num C1) (name VBAT_RF) (type power_in))
        (pin (num C2) (name VDDANA) (type power_in))
        (pin (num C3) (name PB03) (type BiDi))
        (pin (num C4) (name PA05) (type BiDi))
        (pin (num C5) (name PA30) (type BiDi))
        (pin (num C6) (name PA28) (type BiDi))
        (pin (num C7) (name PB23) (type BiDi))
        (pin (num C8) (name PA25) (type BiDi))
        (pin (num D1) (name VR_PA) (type power_out))
        (pin (num D2) (name RXTX) (type output))
        (pin (num D3) (name PA04) (type BiDi))
        (pin (num D4) (name GND) (type power_in))
        (pin (num D5) (name PA31) (type BiDi))
        (pin (num D6) (name GND) (type power_in))
        (pin (num D7) (name PA23) (type BiDi))
        (pin (num D8) (name PA22) (type BiDi))
        (pin (num E1) (name GND_RF) (type power_in))
        (pin (num E2) (name GNDANA) (type power_in))
        (pin (num E3) (name PA06) (type BiDi))
        (pin (num E4) (name PA27) (type BiDi))
        (pin (num E5) (name PB22) (type BiDi))
        (pin (num E6) (name PA17) (type BiDi))
        (pin (num E7) (name PA18) (type BiDi))
        (pin (num E8) (name PA19) (type BiDi))
        (pin (num F1) (name PA_BOOST) (type output))
        (pin (num F2) (name GND_RF) (type power_in))
        (pin (num F3) (name PA07) (type BiDi))
        (pin (num F4) (name PA08) (type BiDi))
        (pin (num F5) (name PA09) (type BiDi))
        (pin (num F6) (name PA13) (type BiDi))
        (pin (num F7) (name PA16) (type BiDi))
        (pin (num F8) (name PA14) (type BiDi))
        (pin (num G1) (name RFO_LF) (type output))
        (pin (num G2) (name GND_RF) (type power_in))
        (pin (num G3) (name GND_RF) (type power_in))
        (pin (num G4) (name VDDI01) (type power_in))
        (pin (num G5) (name GND_RF) (type power_in))
        (pin (num G6) (name GND_RF) (type power_in))
        (pin (num G7) (name GND_RF) (type power_in))
        (pin (num G8) (name PA15) (type BiDi))
        (pin (num H1) (name RFI_LF) (type input))
        (pin (num H2) (name VR_ANA) (type power_out))
        (pin (num H3) (name VBAT_ANA) (type power_in))
        (pin (num H4) (name VR_DIG) (type power_in))
        (pin (num H5) (name GND_RF) (type power_in))
        (pin (num H6) (name XTA) (type input))
        (pin (num H7) (name XTB) (type output))
        (pin (num H8) (name VBAT_DIG) (type power_in))))
    (libpart (lib Elabdev) (part BGS12SN6)
      (description "Infineon MOS SPDT absorbative switch, DC-6GHz, 40dB isolation at 868MHz, TSNP-6-2")
      (docs https://www.infineon.com/dgdl/Infineon-BGS12SN6-DS-v02_03-EN.pdf)
      (footprints
        (fp TSNP*0.7x1.1mm*P0.4mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) BGS12SN6)
        (field (name Footprint) Elabdev:TSNP-6-2_0.7x1.1mm_P0.4mm))
      (pins
        (pin (num 1) (name RF2) (type passive))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name RF1) (type passive))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name RFC) (type passive))
        (pin (num 6) (name CTRL) (type input))))
    (libpart (lib Elabdev) (part CMM-2718AB-383161)
      (description "MEMS Omnidirectional Digital Microphone, HLGA-3")
      (docs https://www.cui.com/product/resource/cmm-2718ab-383161-tr.pdf)
      (footprints
        (fp HLGA*1.85x2.75mm*P0.95mm*))
      (fields
        (field (name Reference) MIC)
        (field (name Value) CMM-2718AB-383161)
        (field (name Footprint) Elabdev:HLGA-3_1.85x2.75mm_P0.95mm))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name OUT) (type output))
        (pin (num 3) (name GND) (type power_in))))
    (libpart (lib Elabdev) (part Conn_ST_STDC14)
      (description "ST Debug Connector, standard ARM Cortex-M SWD and JTAG interface plus UART")
      (docs https://www.st.com/content/ccc/resource/technical/document/user_manual/group1/99/49/91/b6/b2/3a/46/e5/DM00526767/files/DM00526767.pdf/jcr:content/translations/en.DM00526767.pdf)
      (footprints
        (fp PinHeader?2x07?P1.27mm*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_ST_STDC14))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name NC) (type NotConnected))
        (pin (num 3) (name VCC) (type power_in))
        (pin (num 4) (name JTMS/SWDIO) (type BiDi))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name JCLK/SWCLK) (type output))
        (pin (num 7) (name GND) (type passive))
        (pin (num 8) (name JTDO/SWO) (type input))
        (pin (num 9) (name JRCLK/NC) (type input))
        (pin (num 10) (name JTDI/NC) (type output))
        (pin (num 11) (name GNDDetect) (type passive))
        (pin (num 12) (name ~RST) (type openCol))
        (pin (num 13) (name VCP_RX) (type output))
        (pin (num 14) (name VCP_TX) (type input))))
    (libpart (lib Elabdev) (part ESD9B5.0ST5G)
      (aliases
        (alias ESD9B3.3ST5G)
        (alias SZESD9B5.0ST5G))
      (footprints
        (fp D*SOD?923*))
      (fields
        (field (name Reference) D)
        (field (name Value) ESD9B5.0ST5G)
        (field (name Footprint) Diode_SMD:D_SOD-923))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A2) (type passive))))
    (libpart (lib Elabdev) (part Logofirm)
      (description "Firma Logo")
      (docs ~)
      (fields
        (field (name Reference) LOGO)
        (field (name Value) Logofirm)))
    (libpart (lib Elabdev) (part MASW007935)
      (description "Macom GaAs RF SPDT absorbative switch, DC-3GHz, 1.1/22dB loss/isolation, SOT-26 (SOT-23-6)")
      (docs https://cdn.macom.com/datasheets/MASW-007935.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) MASW007935)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name RF1) (type passive))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name RF2) (type passive))
        (pin (num 4) (name V2) (type input))
        (pin (num 5) (name RFC) (type passive))
        (pin (num 6) (name V1) (type input))))
    (libpart (lib Elabdev) (part SKY13373)
      (description "SP3T DC-6.0GHz switch, 30dB isolation at 2.5GHz, QFN-12")
      (docs http://www.skyworksinc.com/uploads/documents/SKY13373_460LF_201264N.pdf)
      (footprints
        (fp QFN*1EP*2x2*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) SKY13373)
        (field (name Footprint) Elabdev:QFN-12-1EP_2x2mm_P0.5mm_EP0.76x0.76mm))
      (pins
        (pin (num 1) (name J1) (type passive))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name J3) (type passive))
        (pin (num 4) (name V1) (type input))
        (pin (num 5) (name V2) (type input))
        (pin (num 6) (name VDD) (type power_in))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name J2) (type passive))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name RFC) (type passive))
        (pin (num 12) (name GND) (type power_in))))
    (libpart (lib Elabdev) (part STM32WLE5CCU6)
      (aliases
        (alias STM32WLE5C8U6)
        (alias STM32WLE5CBU6))
      (description "LPWAN Arm Cortex-M4 MCUs, LoRa, (G)FSK, (G)MSK, BPSK, 64/128/256KB Flash, 64KB SRAM, 7x7mm UFQFPN-48")
      (docs https://www.st.com/resource/datasheet/stm32wle5jc.pdf)
      (footprints
        (fp QFN*1EP*7x7mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32WLE5CCU6)
        (field (name Footprint) Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm)
        (field (name Datasheet) https://www.st.com/en/microcontrollers-microprocessors/stm32wle5jc.html))
      (pins
        (pin (num 1) (name PB3) (type BiDi))
        (pin (num 2) (name PB4) (type BiDi))
        (pin (num 3) (name PB5) (type BiDi))
        (pin (num 4) (name PB6) (type BiDi))
        (pin (num 5) (name PB7) (type BiDi))
        (pin (num 6) (name PB8) (type BiDi))
        (pin (num 7) (name PA0) (type BiDi))
        (pin (num 8) (name PA1) (type BiDi))
        (pin (num 9) (name PA2) (type BiDi))
        (pin (num 10) (name PA3) (type BiDi))
        (pin (num 11) (name VDD) (type power_in))
        (pin (num 12) (name PA4) (type BiDi))
        (pin (num 13) (name PA5) (type BiDi))
        (pin (num 14) (name PA6) (type BiDi))
        (pin (num 15) (name PA7) (type BiDi))
        (pin (num 16) (name PA8) (type BiDi))
        (pin (num 17) (name PA9) (type BiDi))
        (pin (num 18) (name NRST) (type input))
        (pin (num 19) (name PH3-BOOT0) (type input))
        (pin (num 20) (name RFI_P) (type input))
        (pin (num 21) (name RFI_N) (type input))
        (pin (num 22) (name RFO_LP) (type output))
        (pin (num 23) (name RFO_HP) (type output))
        (pin (num 24) (name VR_PA) (type power_out))
        (pin (num 25) (name VDDPA) (type power_out))
        (pin (num 26) (name OSC_IN) (type input))
        (pin (num 27) (name OSC_OUT) (type output))
        (pin (num 28) (name VDDRF) (type power_in))
        (pin (num 29) (name VDDRF1V55) (type power_in))
        (pin (num 30) (name PB0-VDD_TCXO) (type BiDi))
        (pin (num 31) (name PB2) (type BiDi))
        (pin (num 32) (name PB12) (type BiDi))
        (pin (num 33) (name PA10) (type BiDi))
        (pin (num 34) (name PA11) (type BiDi))
        (pin (num 35) (name PA12) (type BiDi))
        (pin (num 36) (name PA13) (type BiDi))
        (pin (num 37) (name VBAT) (type power_in))
        (pin (num 38) (name PC13) (type BiDi))
        (pin (num 39) (name PC14_OSC32_IN) (type BiDi))
        (pin (num 40) (name PC15_OSC32_OUT) (type BiDi))
        (pin (num 41) (name VDDA) (type power_in))
        (pin (num 42) (name PA14) (type BiDi))
        (pin (num 43) (name PA15) (type BiDi))
        (pin (num 44) (name VDD) (type power_in))
        (pin (num 45) (name VFBSMPS) (type power_in))
        (pin (num 46) (name VDDSMPS) (type power_in))
        (pin (num 47) (name VLXSMPS) (type power_in))
        (pin (num 48) (name VSSSMPS) (type power_in))
        (pin (num 49) (name EP) (type power_in))))
    (libpart (lib Elabdev) (part Soldfeld)
      (description "Solder Area")
      (fields
        (field (name Reference) SF)
        (field (name Value) Soldfeld)
        (field (name Footprint) Elabdev:Solderarea)))
    (libpart (lib Elabdev) (part TPS73533DRV)
      (description "3.3V 500mA, Low Quiescent Current, Low Noise, High PSRR, Low-Dropout Linear Regulator, WSON-6")
      (docs https://www.ti.com/lit/ds/symlink/tps735.pdf)
      (footprints
        (fp Texas*S*PWSON*N*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPS73533DRV)
        (field (name Footprint) Package_SON:Texas_PWSON-N6))
      (pins
        (pin (num 1) (name OUT) (type power_out))
        (pin (num 2) (name NR) (type passive))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name EN) (type input))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name IN) (type power_in))
        (pin (num 7) (name GND) (type power_in))))
    (libpart (lib Elabdev) (part TYETBCSANF)
      (description "32MHz TCXO Clipped Sine Wave Oscillator")
      (docs http://www.taitien.com/wp-content/uploads/2015/12/XO-0081_TY.pdf)
      (footprints
        (fp Oscillator*SMD*2.5*2.0*))
      (fields
        (field (name Reference) XC)
        (field (name Value) TYETBCSANF)
        (field (name Footprint) Elabdev:Oscillator_SMD_Taitien_TY-4Pin_2.5x2.0mm))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type output))
        (pin (num 4) (name VCC) (type power_in))))
    (libpart (lib Jumper) (part Jumper_2_Bridged)
      (description "Jumper, 2-pole, closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_2_Bridged))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_2_Bridged)
      (description "Solder Jumper, 2-pole, closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Bridged))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_2_Open)
      (description "Solder Jumper, 2-pole, open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_3_Bridged12)
      (description "3-pole Solder Jumper, pins 1+2 closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged12*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_3_Bridged12))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive))))
    (libpart (lib Mechanical) (part Fiducial)
      (description "Fiducial Marker")
      (docs ~)
      (footprints
        (fp Fiducial*))
      (fields
        (field (name Reference) FID)
        (field (name Value) Fiducial)))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib Memory_EEPROM) (part 24LC16)
      (aliases
        (alias 24LC02)
        (alias 24LC00)
        (alias 24LC04)
        (alias 24LC08)
        (alias 24LC01)
        (alias 24LC512)
        (alias 24LC64)
        (alias 24LC1025)
        (alias 24LC32)
        (alias 24LC256)
        (alias 24LC128)
        (alias CAT24C256)
        (alias CAT24C128))
      (description "I2C Serial EEPROM, 16Kb, DIP-8/SOIC-8/TSSOP-8/DFN-8")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/21703d.pdf)
      (footprints
        (fp DIP*W7.62mm*)
        (fp SOIC*3.9x4.9mm*)
        (fp TSSOP*4.4x3mm*P0.65mm*)
        (fp DFN*3x2mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 24LC16))
      (pins
        (pin (num 1) (name A0) (type input))
        (pin (num 2) (name A1) (type input))
        (pin (num 3) (name A2) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name SDA) (type BiDi))
        (pin (num 6) (name SCL) (type input))
        (pin (num 7) (name WP) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Power_Protection) (part NUP2202)
      (description "Transient voltage suppressor designed to protect high speed data lines from ESD, EFT, and lightning")
      (docs http://www.onsemi.ru.com/pub_link/Collateral/NUP2202W1-D.PDF)
      (footprints
        (fp SOT?363*))
      (fields
        (field (name Reference) U)
        (field (name Value) NUP2202)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-363_SC-70-6))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type NotConnected))
        (pin (num 4) (name ~) (type NotConnected))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib Power_Protection) (part SP0503BAHT)
      (description "TVS Diode Array, 5.5V Standoff, 3 Channels, SOT-143 package")
      (docs http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf)
      (footprints
        (fp SOT?143*))
      (fields
        (field (name Reference) D)
        (field (name Value) SP0503BAHT)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-143))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))
        (pin (num 3) (name K) (type passive))
        (pin (num 4) (name K) (type passive))))
    (libpart (lib RF_Switch) (part MSWA-2-20)
      (description "SPDT DC-2.0GHz absorbative switch, 50 Ohm, SOP-8")
      (docs https://www.minicircuits.com/pdfs/MSWA-2-20+.pdf)
      (footprints
        (fp SOP*3.76x4.96mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MSWA-2-20)
        (field (name Footprint) Package_SO:SOP-8_3.76x4.96mm_P1.27mm))
      (pins
        (pin (num 1) (name CONTROL2) (type input))
        (pin (num 2) (name RF_IN) (type passive))
        (pin (num 3) (name CONTROL1) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name RF_OUT2) (type passive))
        (pin (num 6) (name GND) (type passive))
        (pin (num 7) (name GND) (type passive))
        (pin (num 8) (name RF_OUT1) (type passive))))
    (libpart (lib Switch) (part SW_SPST)
      (description "Single Pole Single Throw (SPST) switch")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_SPST))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Elabdev)
      (uri libraries/elabdev.lib))
    (library (logical Jumper)
      (uri /usr/share/kicad/library/Jumper.lib))
    (library (logical Mechanical)
      (uri /usr/share/kicad/library/Mechanical.lib))
    (library (logical Memory_EEPROM)
      (uri /usr/share/kicad/library/Memory_EEPROM.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical RF_Switch)
      (uri /usr/share/kicad/library/RF_Switch.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib)))
  (nets
    (net (code 1) (name /Sheet5F53D686/PWR_VDDA)
      (node (ref U14) (pin 41))
      (node (ref L15) (pin 2))
      (node (ref C62) (pin 1))
      (node (ref C64) (pin 1)))
    (net (code 2) (name /Sheet5F53D5B4/XCEIV)
      (node (ref U4) (pin 5))
      (node (ref U3) (pin D2)))
    (net (code 3) (name /Sheet5F53D5B4/HFIN)
      (node (ref L6) (pin 2))
      (node (ref U3) (pin A1)))
    (net (code 4) (name /Sheet5F53D5B4/HFOUT)
      (node (ref C39) (pin 1))
      (node (ref L7) (pin 2))
      (node (ref C35) (pin 1))
      (node (ref U3) (pin B1)))
    (net (code 5) (name /Sheet5F53D5B4/HPOUT)
      (node (ref L4) (pin 2))
      (node (ref U3) (pin F1)))
    (net (code 6) (name /Sheet5F53D5B4/POWAMP)
      (node (ref U3) (pin D1))
      (node (ref L5) (pin 2))
      (node (ref C32) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref L7) (pin 1)))
    (net (code 7) (name /Sheet5F53D5B4/RFSWPWR)
      (node (ref C22) (pin 2))
      (node (ref XC1) (pin 4))
      (node (ref C21) (pin 1))
      (node (ref U4) (pin 6))
      (node (ref U3) (pin F5)))
    (net (code 8) (name /Sheet5F53D5B4/BANDSEL)
      (node (ref U3) (pin F6))
      (node (ref U4) (pin 4)))
    (net (code 9) (name /Sheet5F53D686/PWR_VLXSMPS)
      (node (ref R19) (pin 1))
      (node (ref U14) (pin 47)))
    (net (code 10) (name /Sheet5F53D686/PWR_VDDRF1V55)
      (node (ref U14) (pin 45))
      (node (ref C66) (pin 1))
      (node (ref L16) (pin 2))
      (node (ref U14) (pin 29))
      (node (ref C65) (pin 1)))
    (net (code 11) (name +3V3)
      (node (ref Q1) (pin 1))
      (node (ref MIC1) (pin 1))
      (node (ref C92) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref J3) (pin 17))
      (node (ref C48) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref J3) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref FB1) (pin 1))
      (node (ref U3) (pin A7))
      (node (ref U3) (pin A8))
      (node (ref U14) (pin 46))
      (node (ref U3) (pin G4))
      (node (ref U3) (pin H8))
      (node (ref R2) (pin 1))
      (node (ref JP1) (pin 2))
      (node (ref J17) (pin 1))
      (node (ref J18) (pin 3))
      (node (ref R35) (pin 1))
      (node (ref U14) (pin 11))
      (node (ref U14) (pin 44))
      (node (ref TH1) (pin 1))
      (node (ref U14) (pin 28))
      (node (ref J13) (pin 6))
      (node (ref J14) (pin 7))
      (node (ref U12) (pin 8))
      (node (ref J11) (pin 17))
      (node (ref J11) (pin 1))
      (node (ref U8) (pin 8))
      (node (ref U7) (pin 8))
      (node (ref R13) (pin 1))
      (node (ref U6) (pin 8))
      (node (ref R12) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref C41) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref U9) (pin 8))
      (node (ref C42) (pin 1))
      (node (ref C70) (pin 1))
      (node (ref C72) (pin 1))
      (node (ref C73) (pin 1))
      (node (ref C68) (pin 1))
      (node (ref C71) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref U13) (pin 8))
      (node (ref J12) (pin 11))
      (node (ref J12) (pin 12))
      (node (ref R16) (pin 1))
      (node (ref J16) (pin 1))
      (node (ref J19) (pin 3))
      (node (ref C67) (pin 1))
      (node (ref L15) (pin 1))
      (node (ref C61) (pin 1))
      (node (ref J1) (pin 3))
      (node (ref TP2) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C16) (pin 1)))
    (net (code 12) (name /Sheet5F53D686/PWR_VBAT)
      (node (ref C69) (pin 1))
      (node (ref U14) (pin 37))
      (node (ref BT2) (pin 1)))
    (net (code 13) (name /Sheet5F53D5B4/SWDIO)
      (node (ref U3) (pin D5))
      (node (ref J4) (pin 2)))
    (net (code 14) (name /Sheet5F53D5B4/I2C_SCL)
      (node (ref U8) (pin 6))
      (node (ref U9) (pin 6))
      (node (ref R14) (pin 2))
      (node (ref U3) (pin E6)))
    (net (code 15) (name /Sheet5F53D5B4/I2C_SDA)
      (node (ref R15) (pin 2))
      (node (ref U3) (pin F7))
      (node (ref U8) (pin 5))
      (node (ref U9) (pin 5)))
    (net (code 16) (name /Sheet5F53D5B4/SWDCLK)
      (node (ref J4) (pin 4))
      (node (ref U3) (pin C5)))
    (net (code 17) (name /Sheet5F53D686/IDSC)
      (node (ref JP14) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref U13) (pin 6))
      (node (ref U12) (pin 6))
      (node (ref JP22) (pin 1)))
    (net (code 18) (name /Sheet5F53D686/SW_RFO)
      (node (ref L21) (pin 1))
      (node (ref U10) (pin 5))
      (node (ref U1) (pin 1))
      (node (ref C46) (pin 1))
      (node (ref C89) (pin 1)))
    (net (code 19) (name /Sheet5F53D686/SW_RFI)
      (node (ref C88) (pin 1))
      (node (ref C90) (pin 1))
      (node (ref U10) (pin 8))
      (node (ref U1) (pin 3))
      (node (ref C47) (pin 1)))
    (net (code 20) (name /Sheet5F53D686/RSTX)
      (node (ref R36) (pin 2))
      (node (ref J9) (pin 5))
      (node (ref JP11) (pin 1))
      (node (ref U14) (pin 4)))
    (net (code 21) (name /Sheet5F53D686/RSRX)
      (node (ref R37) (pin 2))
      (node (ref JP12) (pin 1))
      (node (ref U14) (pin 5))
      (node (ref J9) (pin 4)))
    (net (code 22) (name /Sheet5F53D686/IDSD)
      (node (ref U13) (pin 5))
      (node (ref R16) (pin 2))
      (node (ref U12) (pin 5))
      (node (ref JP13) (pin 2))
      (node (ref JP23) (pin 1)))
    (net (code 23) (name /Sheet5F53D686/FE_CTRL2)
      (node (ref U10) (pin 1))
      (node (ref C45) (pin 1))
      (node (ref U11) (pin 4))
      (node (ref U14) (pin 38))
      (node (ref U1) (pin 6)))
    (net (code 24) (name /Sheet5F53D686/SNSD)
      (node (ref J12) (pin 8))
      (node (ref J12) (pin 7))
      (node (ref U14) (pin 43))
      (node (ref J14) (pin 11))
      (node (ref J19) (pin 2)))
    (net (code 25) (name /Sheet5F53D686/SNSC)
      (node (ref J12) (pin 6))
      (node (ref J12) (pin 5))
      (node (ref J19) (pin 1))
      (node (ref U14) (pin 35))
      (node (ref J14) (pin 12)))
    (net (code 26) (name GND)
      (node (ref J3) (pin 25))
      (node (ref J2) (pin B1))
      (node (ref J2) (pin B12))
      (node (ref J3) (pin 39))
      (node (ref J3) (pin 34))
      (node (ref J7) (pin 2))
      (node (ref J3) (pin 30))
      (node (ref J3) (pin 9))
      (node (ref J3) (pin 6))
      (node (ref C48) (pin 2))
      (node (ref U10) (pin 7))
      (node (ref U10) (pin 6))
      (node (ref U10) (pin 4))
      (node (ref U11) (pin 2))
      (node (ref U6) (pin 3))
      (node (ref C55) (pin 2))
      (node (ref TP1) (pin 1))
      (node (ref C57) (pin 2))
      (node (ref C53) (pin 2))
      (node (ref C58) (pin 2))
      (node (ref C54) (pin 2))
      (node (ref U9) (pin 4))
      (node (ref C43) (pin 2))
      (node (ref C59) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref C45) (pin 2))
      (node (ref J8) (pin 2))
      (node (ref U4) (pin 8))
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 2))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 10))
      (node (ref C30) (pin 2))
      (node (ref C41) (pin 2))
      (node (ref U7) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref AE2) (pin 2))
      (node (ref U7) (pin 2))
      (node (ref U7) (pin 3))
      (node (ref C32) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref U7) (pin 4))
      (node (ref R32) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref C38) (pin 2))
      (node (ref AE4) (pin 2))
      (node (ref AE7) (pin 2))
      (node (ref AE6) (pin 2))
      (node (ref AE3) (pin 1))
      (node (ref U6) (pin 2))
      (node (ref U6) (pin 4))
      (node (ref C60) (pin 2))
      (node (ref C56) (pin 2))
      (node (ref AE8) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref U6) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref C65) (pin 2))
      (node (ref U12) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref C66) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref U13) (pin 1))
      (node (ref U13) (pin 4))
      (node (ref U13) (pin 3))
      (node (ref U13) (pin 2))
      (node (ref C61) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C64) (pin 2))
      (node (ref C62) (pin 2))
      (node (ref C69) (pin 2))
      (node (ref U12) (pin 1))
      (node (ref BT2) (pin 2))
      (node (ref J11) (pin 25))
      (node (ref C73) (pin 2))
      (node (ref C72) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref J11) (pin 20))
      (node (ref C67) (pin 2))
      (node (ref J15) (pin 2))
      (node (ref C63) (pin 2))
      (node (ref J13) (pin 5))
      (node (ref J12) (pin 9))
      (node (ref J12) (pin 10))
      (node (ref U12) (pin 3))
      (node (ref U12) (pin 4))
      (node (ref J19) (pin 4))
      (node (ref J16) (pin 4))
      (node (ref J11) (pin 9))
      (node (ref J14) (pin 8))
      (node (ref J14) (pin 9))
      (node (ref J11) (pin 14))
      (node (ref J9) (pin 1))
      (node (ref C40) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref J2) (pin A1))
      (node (ref J2) (pin A12))
      (node (ref U5) (pin 2))
      (node (ref C42) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref J4) (pin 3))
      (node (ref J3) (pin 20))
      (node (ref J5) (pin 1))
      (node (ref C8) (pin 2))
      (node (ref J3) (pin 14))
      (node (ref J4) (pin 5))
      (node (ref J4) (pin 9))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 7))
      (node (ref J11) (pin 30))
      (node (ref C70) (pin 2))
      (node (ref J11) (pin 34))
      (node (ref C71) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref J11) (pin 6))
      (node (ref J11) (pin 39))
      (node (ref C16) (pin 2))
      (node (ref C68) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref U8) (pin 4))
      (node (ref BT1) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C86) (pin 2))
      (node (ref C81) (pin 2))
      (node (ref XC1) (pin 2))
      (node (ref C82) (pin 2))
      (node (ref C75) (pin 1))
      (node (ref U14) (pin 49))
      (node (ref C9) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U14) (pin 48))
      (node (ref C89) (pin 2))
      (node (ref C74) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref SW3) (pin 1))
      (node (ref R31) (pin 1))
      (node (ref J17) (pin 3))
      (node (ref J17) (pin 5))
      (node (ref R33) (pin 2))
      (node (ref R38) (pin 2))
      (node (ref SW4) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref C91) (pin 2))
      (node (ref SW6) (pin 2))
      (node (ref Y2) (pin 2))
      (node (ref Y2) (pin 4))
      (node (ref C76) (pin 1))
      (node (ref C90) (pin 2))
      (node (ref C77) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref J18) (pin 5))
      (node (ref J18) (pin 7))
      (node (ref SW5) (pin 1))
      (node (ref U3) (pin G5))
      (node (ref U3) (pin G2))
      (node (ref U3) (pin G3))
      (node (ref C19) (pin 1))
      (node (ref U3) (pin G6))
      (node (ref U3) (pin G7))
      (node (ref C92) (pin 2))
      (node (ref U3) (pin H5))
      (node (ref C17) (pin 2))
      (node (ref U3) (pin E1))
      (node (ref R34) (pin 2))
      (node (ref U3) (pin D4))
      (node (ref U3) (pin D6))
      (node (ref U3) (pin E2))
      (node (ref U3) (pin F2))
      (node (ref MIC1) (pin 3))
      (node (ref U3) (pin A2))
      (node (ref U3) (pin B2))
      (node (ref U3) (pin B3))
      (node (ref U3) (pin B5))
      (node (ref U3) (pin B7))
      (node (ref C85) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C83) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C14) (pin 2)))
    (net (code 27) (name /Sheet5F53D686/FE_CTRL1)
      (node (ref U10) (pin 3))
      (node (ref U11) (pin 6))
      (node (ref U14) (pin 32))
      (node (ref C43) (pin 1)))
    (net (code 28) (name /Sheet5F53D686/PWR_VDDPA)
      (node (ref C63) (pin 1))
      (node (ref U14) (pin 25)))
    (net (code 29) (name "Net-(TP4-Pad1)")
      (node (ref TP6) (pin 1))
      (node (ref TP4) (pin 1)))
    (net (code 30) (name "Net-(TP3-Pad1)")
      (node (ref TP3) (pin 1))
      (node (ref TP5) (pin 1)))
    (net (code 31) (name /Sheet5F53D5B4/USB_N)
      (node (ref U3) (pin B8))
      (node (ref U5) (pin 6))
      (node (ref J2) (pin A7))
      (node (ref J2) (pin B7)))
    (net (code 32) (name /Sheet60040980/ID_SC)
      (node (ref U6) (pin 6))
      (node (ref J3) (pin 28))
      (node (ref R12) (pin 2))
      (node (ref U7) (pin 6)))
    (net (code 33) (name /Sheet60040980/ID_SD)
      (node (ref R11) (pin 2))
      (node (ref J3) (pin 27))
      (node (ref U6) (pin 5))
      (node (ref U7) (pin 5)))
    (net (code 34) (name /Sheet5F53D5B4/USB_BUS)
      (node (ref U2) (pin 6))
      (node (ref C5) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref R5) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref U3) (pin F3)))
    (net (code 35) (name /Sheet5F53D5B4/USB_P)
      (node (ref U5) (pin 1))
      (node (ref J2) (pin A6))
      (node (ref U3) (pin C8))
      (node (ref J2) (pin B6)))
    (net (code 36) (name /Sheet5F53D5B4/UART_TX)
      (node (ref J5) (pin 5))
      (node (ref U3) (pin D3))
      (node (ref JP2) (pin 1)))
    (net (code 37) (name /Sheet5F53D5B4/UART_RX)
      (node (ref JP3) (pin 1))
      (node (ref J5) (pin 4))
      (node (ref U3) (pin C4)))
    (net (code 38) (name /Sheet5F53D5B4/CMDRST)
      (node (ref SW1) (pin 1))
      (node (ref U3) (pin B6))
      (node (ref R9) (pin 2))
      (node (ref J4) (pin 10))
      (node (ref C20) (pin 1)))
    (net (code 39) (name "Net-(R3-Pad1)")
      (node (ref SW1) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 40) (name "Net-(U3-PadG1)")
      (node (ref U3) (pin G1)))
    (net (code 41) (name "Net-(U3-PadH1)")
      (node (ref U3) (pin H1)))
    (net (code 42) (name /Sheet5F53D5B4/CRYSTAL_XOUT-RESERVED)
      (node (ref U3) (pin G8)))
    (net (code 43) (name /Sheet5F53D5B4/CRYSTAL_XIN-RESERVED)
      (node (ref U3) (pin F8)))
    (net (code 44) (name "Net-(U3-PadF4)")
      (node (ref U3) (pin F4)))
    (net (code 45) (name "Net-(U3-PadE5)")
      (node (ref U3) (pin E5)))
    (net (code 46) (name "Net-(U3-PadE4)")
      (node (ref U3) (pin E4)))
    (net (code 47) (name "Net-(U3-PadE3)")
      (node (ref U3) (pin E3)))
    (net (code 48) (name /Sheet5F53D5B4/CN_VBAT)
      (node (ref J1) (pin 2))
      (node (ref U3) (pin C3)))
    (net (code 49) (name "Net-(U3-PadD8)")
      (node (ref U3) (pin D8)))
    (net (code 50) (name "Net-(C1-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref U3) (pin H3))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U3) (pin C2))
      (node (ref U3) (pin C1))
      (node (ref C9) (pin 1))
      (node (ref FB1) (pin 2)))
    (net (code 51) (name "Net-(U3-PadB4)")
      (node (ref U3) (pin B4)))
    (net (code 52) (name "Net-(U3-PadC7)")
      (node (ref U3) (pin C7)))
    (net (code 53) (name "Net-(U3-PadD7)")
      (node (ref U3) (pin D7)))
    (net (code 54) (name "Net-(BT1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref BT1) (pin 1)))
    (net (code 55) (name "Net-(R4-Pad2)")
      (node (ref SW2) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 56) (name "Net-(U2-Pad5)")
      (node (ref U2) (pin 5)))
    (net (code 57) (name "Net-(C8-Pad1)")
      (node (ref C8) (pin 1))
      (node (ref U2) (pin 2)))
    (net (code 58) (name "Net-(C7-Pad1)")
      (node (ref JP1) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U2) (pin 1)))
    (net (code 59) (name "Net-(C18-Pad2)")
      (node (ref Y1) (pin 1))
      (node (ref C18) (pin 2))
      (node (ref U3) (pin A3)))
    (net (code 60) (name "Net-(XC1-Pad1)")
      (node (ref XC1) (pin 1)))
    (net (code 61) (name "Net-(C14-Pad1)")
      (node (ref U3) (pin H2))
      (node (ref C15) (pin 1))
      (node (ref C14) (pin 1)))
    (net (code 62) (name "Net-(C17-Pad1)")
      (node (ref C17) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref U3) (pin A5)))
    (net (code 63) (name "Net-(L1-Pad2)")
      (node (ref L1) (pin 2))
      (node (ref U3) (pin A6)))
    (net (code 64) (name "Net-(R4-Pad1)")
      (node (ref U3) (pin C6))
      (node (ref R4) (pin 1)))
    (net (code 65) (name "Net-(C19-Pad2)")
      (node (ref Y1) (pin 2))
      (node (ref U3) (pin A4))
      (node (ref C19) (pin 2)))
    (net (code 66) (name "Net-(U3-PadH6)")
      (node (ref U3) (pin H6))
      (node (ref XC1) (pin 3)))
    (net (code 67) (name "Net-(U3-PadH7)")
      (node (ref U3) (pin H7)))
    (net (code 68) (name "Net-(C13-Pad1)")
      (node (ref U3) (pin H4))
      (node (ref C13) (pin 1)))
    (net (code 69) (name "Net-(D1-Pad1)")
      (node (ref U3) (pin E7))
      (node (ref D1) (pin 1)))
    (net (code 70) (name "Net-(D2-Pad1)")
      (node (ref U3) (pin E8))
      (node (ref D2) (pin 1)))
    (net (code 71) (name "Net-(D1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 72) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 73) (name "Net-(U14-Pad12)")
      (node (ref U14) (pin 12)))
    (net (code 74) (name "Net-(U14-Pad10)")
      (node (ref U14) (pin 10)))
    (net (code 75) (name /Sheet5F53D686/T_SWD)
      (node (ref U14) (pin 1))
      (node (ref R23) (pin 2)))
    (net (code 76) (name "Net-(U14-Pad6)")
      (node (ref U14) (pin 6)))
    (net (code 77) (name "Net-(C93-Pad2)")
      (node (ref C93) (pin 2))
      (node (ref U14) (pin 3)))
    (net (code 78) (name "Net-(U14-Pad2)")
      (node (ref U14) (pin 2)))
    (net (code 79) (name /Sheet5F53D686/T_CLK)
      (node (ref U14) (pin 42))
      (node (ref R21) (pin 2)))
    (net (code 80) (name "Net-(R29-Pad2)")
      (node (ref U14) (pin 14))
      (node (ref R29) (pin 2)))
    (net (code 81) (name "Net-(R30-Pad2)")
      (node (ref R30) (pin 2))
      (node (ref U14) (pin 15)))
    (net (code 82) (name "Net-(U14-Pad16)")
      (node (ref U14) (pin 16)))
    (net (code 83) (name "Net-(R28-Pad2)")
      (node (ref R28) (pin 2))
      (node (ref U14) (pin 13)))
    (net (code 84) (name /Sheet5F53D686/T_DIO)
      (node (ref U14) (pin 36))
      (node (ref R22) (pin 2)))
    (net (code 85) (name /Sheet5F53D686/CONN_TDI)
      (node (ref J17) (pin 8))
      (node (ref J18) (pin 10))
      (node (ref R24) (pin 1)))
    (net (code 86) (name "Net-(U14-Pad30)")
      (node (ref U14) (pin 30)))
    (net (code 87) (name "Net-(C75-Pad2)")
      (node (ref U14) (pin 27))
      (node (ref Y2) (pin 3))
      (node (ref C75) (pin 2)))
    (net (code 88) (name "Net-(C77-Pad2)")
      (node (ref Y3) (pin 1))
      (node (ref U14) (pin 40))
      (node (ref C77) (pin 2)))
    (net (code 89) (name "Net-(C76-Pad2)")
      (node (ref Y3) (pin 2))
      (node (ref U14) (pin 39))
      (node (ref C76) (pin 2)))
    (net (code 90) (name "Net-(JP25-Pad2)")
      (node (ref L17) (pin 2))
      (node (ref JP25) (pin 2)))
    (net (code 91) (name "Net-(JP25-Pad1)")
      (node (ref U14) (pin 23))
      (node (ref JP25) (pin 1)))
    (net (code 92) (name "Net-(JP25-Pad3)")
      (node (ref U14) (pin 22))
      (node (ref JP25) (pin 3)))
    (net (code 93) (name /Sheet5F53D686/DEJIT2)
      (node (ref D6) (pin 3))
      (node (ref R26) (pin 2))
      (node (ref C79) (pin 1))
      (node (ref SW4) (pin 2)))
    (net (code 94) (name "Net-(C78-Pad2)")
      (node (ref C80) (pin 2))
      (node (ref C79) (pin 2))
      (node (ref D6) (pin 1))
      (node (ref C78) (pin 2)))
    (net (code 95) (name /Sheet5F53D686/DEJIT3)
      (node (ref C80) (pin 1))
      (node (ref R27) (pin 2))
      (node (ref SW5) (pin 2))
      (node (ref D6) (pin 2)))
    (net (code 96) (name "Net-(D5-Pad2)")
      (node (ref R30) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 97) (name /Sheet5F53D686/DEJIT1)
      (node (ref R25) (pin 2))
      (node (ref SW3) (pin 2))
      (node (ref D6) (pin 4))
      (node (ref C78) (pin 1)))
    (net (code 98) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref R29) (pin 1)))
    (net (code 99) (name "Net-(D3-Pad2)")
      (node (ref R28) (pin 1))
      (node (ref D3) (pin 2)))
    (net (code 100) (name /Sheet5F53D686/BTN3)
      (node (ref U14) (pin 9))
      (node (ref R27) (pin 1)))
    (net (code 101) (name /Sheet5F53D686/BTN1)
      (node (ref R25) (pin 1))
      (node (ref U14) (pin 7)))
    (net (code 102) (name /Sheet5F53D686/BTN2)
      (node (ref U14) (pin 8))
      (node (ref R26) (pin 1)))
    (net (code 103) (name "Net-(J18-Pad9)")
      (node (ref J18) (pin 9)))
    (net (code 104) (name "Net-(J17-Pad9)")
      (node (ref R33) (pin 1))
      (node (ref J17) (pin 9)))
    (net (code 105) (name "Net-(J18-Pad13)")
      (node (ref R36) (pin 1))
      (node (ref J18) (pin 13)))
    (net (code 106) (name "Net-(J18-Pad11)")
      (node (ref R38) (pin 1))
      (node (ref J18) (pin 11)))
    (net (code 107) (name "Net-(J17-Pad7)")
      (node (ref J17) (pin 7)))
    (net (code 108) (name /Sheet5F53D686/CONN_SWD)
      (node (ref J18) (pin 8))
      (node (ref J17) (pin 6))
      (node (ref R23) (pin 1)))
    (net (code 109) (name /Sheet5F53D686/CONN_DIO)
      (node (ref R22) (pin 1))
      (node (ref J18) (pin 4))
      (node (ref J17) (pin 2)))
    (net (code 110) (name /Sheet5F53D686/CONN_CLK)
      (node (ref J18) (pin 6))
      (node (ref J17) (pin 4))
      (node (ref R21) (pin 1)))
    (net (code 111) (name /Sheet5F53D686/T_NRST)
      (node (ref U14) (pin 18))
      (node (ref SW6) (pin 1))
      (node (ref D7) (pin 2))
      (node (ref C91) (pin 1))
      (node (ref R20) (pin 2)))
    (net (code 112) (name /Sheet5F53D686/CONN_NRST)
      (node (ref J17) (pin 10))
      (node (ref R35) (pin 2))
      (node (ref R20) (pin 1))
      (node (ref J18) (pin 12)))
    (net (code 113) (name "Net-(J18-Pad14)")
      (node (ref J18) (pin 14))
      (node (ref R37) (pin 1)))
    (net (code 114) (name "Net-(JP24-Pad2)")
      (node (ref R31) (pin 2))
      (node (ref JP24) (pin 2)))
    (net (code 115) (name "Net-(JP24-Pad1)")
      (node (ref JP24) (pin 1))
      (node (ref U14) (pin 19)))
    (net (code 116) (name "Net-(J18-Pad2)")
      (node (ref J18) (pin 2)))
    (net (code 117) (name "Net-(J18-Pad1)")
      (node (ref J18) (pin 1)))
    (net (code 118) (name "Net-(C87-Pad2)")
      (node (ref C87) (pin 2))
      (node (ref L21) (pin 2)))
    (net (code 119) (name "Net-(C84-Pad1)")
      (node (ref C84) (pin 1))
      (node (ref L20) (pin 1))
      (node (ref C87) (pin 1))
      (node (ref C85) (pin 1)))
    (net (code 120) (name "Net-(C86-Pad1)")
      (node (ref C86) (pin 1))
      (node (ref L19) (pin 1))
      (node (ref C88) (pin 2))
      (node (ref U14) (pin 21)))
    (net (code 121) (name "Net-(L19-Pad2)")
      (node (ref L19) (pin 2))
      (node (ref U14) (pin 20)))
    (net (code 122) (name "Net-(C74-Pad2)")
      (node (ref U14) (pin 26))
      (node (ref Y2) (pin 1))
      (node (ref C74) (pin 2)))
    (net (code 123) (name "Net-(C81-Pad1)")
      (node (ref U14) (pin 24))
      (node (ref L18) (pin 2))
      (node (ref C81) (pin 1))
      (node (ref C82) (pin 1)))
    (net (code 124) (name "Net-(C83-Pad1)")
      (node (ref L18) (pin 1))
      (node (ref C84) (pin 2))
      (node (ref L17) (pin 1))
      (node (ref C83) (pin 1))
      (node (ref L20) (pin 2)))
    (net (code 125) (name /Sheet5F53D686/V_NTC)
      (node (ref U14) (pin 34))
      (node (ref TH1) (pin 2))
      (node (ref R32) (pin 1)))
    (net (code 126) (name /Sheet5F53D686/T_TDI)
      (node (ref R24) (pin 2)))
    (net (code 127) (name /Sheet5F53D686/V_ALS)
      (node (ref U14) (pin 31))
      (node (ref Q1) (pin 2))
      (node (ref R34) (pin 1)))
    (net (code 128) (name "Net-(C93-Pad1)")
      (node (ref MIC1) (pin 2))
      (node (ref C93) (pin 1)))
    (net (code 129) (name /Sheet5F53D686/T_SDA1)
      (node (ref JP23) (pin 2))
      (node (ref U14) (pin 33)))
    (net (code 130) (name /Sheet5F53D686/T_SCL1)
      (node (ref JP22) (pin 2))
      (node (ref U14) (pin 17)))
    (net (code 131) (name "Net-(C33-Pad1)")
      (node (ref L8) (pin 2))
      (node (ref L9) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref C34) (pin 2))
      (node (ref C33) (pin 1)))
    (net (code 132) (name "Net-(C33-Pad2)")
      (node (ref C33) (pin 2))
      (node (ref L8) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref U4) (pin 3)))
    (net (code 133) (name "Net-(C35-Pad2)")
      (node (ref C35) (pin 2))
      (node (ref L10) (pin 2)))
    (net (code 134) (name "Net-(C34-Pad1)")
      (node (ref C34) (pin 1))
      (node (ref C38) (pin 1))
      (node (ref L9) (pin 2))
      (node (ref L10) (pin 1)))
    (net (code 135) (name "Net-(C24-Pad2)")
      (node (ref C27) (pin 1))
      (node (ref L3) (pin 2))
      (node (ref C24) (pin 2)))
    (net (code 136) (name "Net-(C23-Pad1)")
      (node (ref L3) (pin 1))
      (node (ref C23) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref L2) (pin 2)))
    (net (code 137) (name "Net-(AE2-Pad1)")
      (node (ref JP6) (pin 2))
      (node (ref AE2) (pin 1)))
    (net (code 138) (name "Net-(C23-Pad2)")
      (node (ref C25) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref L2) (pin 1))
      (node (ref C23) (pin 2)))
    (net (code 139) (name "Net-(C29-Pad2)")
      (node (ref U4) (pin 9))
      (node (ref C29) (pin 2)))
    (net (code 140) (name "Net-(C29-Pad1)")
      (node (ref C30) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref L6) (pin 1)))
    (net (code 141) (name "Net-(C24-Pad1)")
      (node (ref L4) (pin 1))
      (node (ref L5) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref C28) (pin 1)))
    (net (code 142) (name "Net-(JP10-Pad1)")
      (node (ref JP4) (pin 2))
      (node (ref JP6) (pin 1))
      (node (ref JP5) (pin 2))
      (node (ref JP8) (pin 1))
      (node (ref JP10) (pin 1))
      (node (ref U4) (pin 11))
      (node (ref JP7) (pin 2))
      (node (ref JP9) (pin 1)))
    (net (code 143) (name "Net-(AE6-Pad1)")
      (node (ref AE6) (pin 1))
      (node (ref JP9) (pin 2)))
    (net (code 144) (name "Net-(AE5-Pad1)")
      (node (ref AE5) (pin 1))
      (node (ref JP7) (pin 1)))
    (net (code 145) (name "Net-(AE4-Pad1)")
      (node (ref AE4) (pin 1))
      (node (ref JP8) (pin 2)))
    (net (code 146) (name "Net-(AE5-Pad2)")
      (node (ref AE5) (pin 2)))
    (net (code 147) (name "Net-(AE1-Pad1)")
      (node (ref AE1) (pin 1))
      (node (ref JP4) (pin 1)))
    (net (code 148) (name "Net-(AE7-Pad1)")
      (node (ref AE7) (pin 1))
      (node (ref JP10) (pin 2)))
    (net (code 149) (name "Net-(AE3-Pad2)")
      (node (ref AE3) (pin 2))
      (node (ref JP5) (pin 1)))
    (net (code 150) (name "Net-(AE10-Pad1)")
      (node (ref AE10) (pin 1)))
    (net (code 151) (name /Sheet5F84A570/ANT)
      (node (ref C49) (pin 2))
      (node (ref C52) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref C51) (pin 2))
      (node (ref U10) (pin 2))
      (node (ref C44) (pin 2))
      (node (ref C50) (pin 2)))
    (net (code 152) (name "Net-(C57-Pad1)")
      (node (ref C57) (pin 1))
      (node (ref L11) (pin 2))
      (node (ref J8) (pin 1)))
    (net (code 153) (name "Net-(C52-Pad1)")
      (node (ref C52) (pin 1))
      (node (ref L14) (pin 1))
      (node (ref C56) (pin 1)))
    (net (code 154) (name "Net-(AE9-Pad1)")
      (node (ref L14) (pin 2))
      (node (ref C60) (pin 1))
      (node (ref AE9) (pin 1)))
    (net (code 155) (name "Net-(C46-Pad2)")
      (node (ref C46) (pin 2))
      (node (ref U11) (pin 1)))
    (net (code 156) (name "Net-(C47-Pad2)")
      (node (ref U11) (pin 3))
      (node (ref C47) (pin 2)))
    (net (code 157) (name "Net-(C44-Pad1)")
      (node (ref C44) (pin 1))
      (node (ref U11) (pin 5)))
    (net (code 158) (name "Net-(AE10-Pad2)")
      (node (ref L13) (pin 2))
      (node (ref C59) (pin 1))
      (node (ref AE10) (pin 2)))
    (net (code 159) (name "Net-(C51-Pad1)")
      (node (ref C55) (pin 1))
      (node (ref L13) (pin 1))
      (node (ref C51) (pin 1)))
    (net (code 160) (name "Net-(C49-Pad1)")
      (node (ref L11) (pin 1))
      (node (ref C53) (pin 1))
      (node (ref C49) (pin 1)))
    (net (code 161) (name "Net-(AE8-Pad1)")
      (node (ref C58) (pin 1))
      (node (ref AE8) (pin 1))
      (node (ref L12) (pin 2)))
    (net (code 162) (name "Net-(C50-Pad1)")
      (node (ref L12) (pin 1))
      (node (ref C50) (pin 1))
      (node (ref C54) (pin 1)))
    (net (code 163) (name "Net-(J3-Pad38)")
      (node (ref J3) (pin 38)))
    (net (code 164) (name "Net-(J3-Pad5)")
      (node (ref J3) (pin 5)))
    (net (code 165) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7)))
    (net (code 166) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3)))
    (net (code 167) (name "Net-(J3-Pad40)")
      (node (ref J3) (pin 40)))
    (net (code 168) (name "Net-(J3-Pad29)")
      (node (ref J3) (pin 29)))
    (net (code 169) (name "Net-(J3-Pad31)")
      (node (ref J3) (pin 31)))
    (net (code 170) (name "Net-(J3-Pad26)")
      (node (ref J3) (pin 26)))
    (net (code 171) (name "Net-(J3-Pad24)")
      (node (ref J3) (pin 24)))
    (net (code 172) (name "Net-(J3-Pad21)")
      (node (ref J3) (pin 21)))
    (net (code 173) (name "Net-(J3-Pad19)")
      (node (ref J3) (pin 19)))
    (net (code 174) (name "Net-(J3-Pad23)")
      (node (ref J3) (pin 23)))
    (net (code 175) (name "Net-(J3-Pad33)")
      (node (ref J3) (pin 33)))
    (net (code 176) (name "Net-(J3-Pad32)")
      (node (ref J3) (pin 32)))
    (net (code 177) (name "Net-(J3-Pad35)")
      (node (ref J3) (pin 35)))
    (net (code 178) (name "Net-(J3-Pad36)")
      (node (ref J3) (pin 36)))
    (net (code 179) (name "Net-(J3-Pad37)")
      (node (ref J3) (pin 37)))
    (net (code 180) (name "Net-(J3-Pad4)")
      (node (ref J3) (pin 4)))
    (net (code 181) (name "Net-(J2-PadB8)")
      (node (ref J2) (pin B8)))
    (net (code 182) (name "Net-(J6-Pad6)")
      (node (ref J6) (pin 6)))
    (net (code 183) (name "Net-(J6-Pad5)")
      (node (ref J6) (pin 5)))
    (net (code 184) (name "Net-(J6-Pad4)")
      (node (ref J6) (pin 4)))
    (net (code 185) (name "Net-(J6-Pad3)")
      (node (ref J6) (pin 3)))
    (net (code 186) (name "Net-(J6-Pad2)")
      (node (ref J6) (pin 2)))
    (net (code 187) (name "Net-(J6-Pad1)")
      (node (ref J6) (pin 1)))
    (net (code 188) (name "Net-(C40-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref C40) (pin 1))
      (node (ref J2) (pin S1)))
    (net (code 189) (name "Net-(J6-Pad7)")
      (node (ref J6) (pin 7)))
    (net (code 190) (name "Net-(J2-PadB5)")
      (node (ref R7) (pin 1))
      (node (ref J2) (pin B5)))
    (net (code 191) (name "Net-(J2-PadA8)")
      (node (ref J2) (pin A8)))
    (net (code 192) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2)))
    (net (code 193) (name "Net-(J3-Pad11)")
      (node (ref J3) (pin 11)))
    (net (code 194) (name "Net-(J3-Pad12)")
      (node (ref J3) (pin 12)))
    (net (code 195) (name "Net-(J5-Pad3)")
      (node (ref J5) (pin 3)))
    (net (code 196) (name "Net-(J6-Pad8)")
      (node (ref J6) (pin 8)))
    (net (code 197) (name "Net-(J4-Pad8)")
      (node (ref J4) (pin 8)))
    (net (code 198) (name "Net-(J4-Pad7)")
      (node (ref J4) (pin 7)))
    (net (code 199) (name "Net-(J4-Pad6)")
      (node (ref J4) (pin 6)))
    (net (code 200) (name "Net-(J3-Pad18)")
      (node (ref J3) (pin 18)))
    (net (code 201) (name "Net-(J3-Pad16)")
      (node (ref J3) (pin 16)))
    (net (code 202) (name "Net-(J3-Pad15)")
      (node (ref J3) (pin 15)))
    (net (code 203) (name "Net-(J3-Pad13)")
      (node (ref J3) (pin 13)))
    (net (code 204) (name "Net-(J3-Pad10)")
      (node (ref JP3) (pin 2))
      (node (ref J3) (pin 10)))
    (net (code 205) (name "Net-(J5-Pad6)")
      (node (ref J5) (pin 6)))
    (net (code 206) (name "Net-(J5-Pad2)")
      (node (ref J5) (pin 2)))
    (net (code 207) (name "Net-(J3-Pad22)")
      (node (ref J3) (pin 22)))
    (net (code 208) (name "Net-(J3-Pad8)")
      (node (ref J3) (pin 8))
      (node (ref JP2) (pin 2)))
    (net (code 209) (name "Net-(U5-Pad4)")
      (node (ref U5) (pin 4)))
    (net (code 210) (name "Net-(U5-Pad3)")
      (node (ref U5) (pin 3)))
    (net (code 211) (name "Net-(J2-PadA5)")
      (node (ref R8) (pin 1))
      (node (ref J2) (pin A5)))
    (net (code 212) (name "Net-(J2-PadA4)")
      (node (ref R5) (pin 2))
      (node (ref J2) (pin A9))
      (node (ref J2) (pin B4))
      (node (ref J2) (pin A4))
      (node (ref J2) (pin B9))
      (node (ref U5) (pin 5)))
    (net (code 213) (name "Net-(L16-Pad1)")
      (node (ref R19) (pin 2))
      (node (ref L16) (pin 1)))
    (net (code 214) (name "Net-(J14-Pad15)")
      (node (ref J14) (pin 15)))
    (net (code 215) (name "Net-(J14-Pad14)")
      (node (ref J14) (pin 14)))
    (net (code 216) (name "Net-(J14-Pad13)")
      (node (ref J14) (pin 13)))
    (net (code 217) (name "Net-(J14-Pad10)")
      (node (ref J14) (pin 10)))
    (net (code 218) (name "Net-(J12-Pad1)")
      (node (ref J12) (pin 1)))
    (net (code 219) (name "Net-(J12-Pad2)")
      (node (ref J12) (pin 2)))
    (net (code 220) (name "Net-(J12-Pad3)")
      (node (ref J12) (pin 3)))
    (net (code 221) (name "Net-(J12-Pad4)")
      (node (ref J12) (pin 4)))
    (net (code 222) (name "Net-(J14-Pad16)")
      (node (ref J14) (pin 16)))
    (net (code 223) (name "Net-(J11-Pad8)")
      (node (ref J11) (pin 8))
      (node (ref JP11) (pin 2)))
    (net (code 224) (name "Net-(JP19-Pad1)")
      (node (ref JP19) (pin 1)))
    (net (code 225) (name "Net-(J14-Pad2)")
      (node (ref JP19) (pin 2))
      (node (ref J14) (pin 2)))
    (net (code 226) (name "Net-(JP15-Pad1)")
      (node (ref JP15) (pin 1)))
    (net (code 227) (name "Net-(J13-Pad1)")
      (node (ref JP15) (pin 2))
      (node (ref J13) (pin 1)))
    (net (code 228) (name "Net-(JP16-Pad1)")
      (node (ref JP16) (pin 1)))
    (net (code 229) (name "Net-(J13-Pad2)")
      (node (ref JP16) (pin 2))
      (node (ref J13) (pin 2)))
    (net (code 230) (name "Net-(JP17-Pad1)")
      (node (ref JP17) (pin 1)))
    (net (code 231) (name "Net-(J13-Pad3)")
      (node (ref J13) (pin 3))
      (node (ref JP17) (pin 2)))
    (net (code 232) (name "Net-(JP18-Pad1)")
      (node (ref JP18) (pin 1)))
    (net (code 233) (name "Net-(J13-Pad4)")
      (node (ref J13) (pin 4))
      (node (ref JP18) (pin 2)))
    (net (code 234) (name "Net-(J16-Pad2)")
      (node (ref J16) (pin 2))
      (node (ref JP20) (pin 2)))
    (net (code 235) (name "Net-(J14-Pad1)")
      (node (ref J14) (pin 1)))
    (net (code 236) (name "Net-(J14-Pad3)")
      (node (ref J14) (pin 3)))
    (net (code 237) (name "Net-(J14-Pad4)")
      (node (ref J14) (pin 4)))
    (net (code 238) (name "Net-(J14-Pad5)")
      (node (ref J14) (pin 5)))
    (net (code 239) (name "Net-(J14-Pad6)")
      (node (ref J14) (pin 6)))
    (net (code 240) (name "Net-(J11-Pad32)")
      (node (ref J11) (pin 32)))
    (net (code 241) (name "Net-(J11-Pad4)")
      (node (ref J11) (pin 4)))
    (net (code 242) (name "Net-(J11-Pad2)")
      (node (ref J11) (pin 2)))
    (net (code 243) (name "Net-(J11-Pad33)")
      (node (ref J11) (pin 33)))
    (net (code 244) (name "Net-(J9-Pad3)")
      (node (ref J9) (pin 3)))
    (net (code 245) (name "Net-(J11-Pad23)")
      (node (ref J11) (pin 23)))
    (net (code 246) (name "Net-(J11-Pad19)")
      (node (ref J11) (pin 19)))
    (net (code 247) (name "Net-(J11-Pad21)")
      (node (ref J11) (pin 21)))
    (net (code 248) (name "Net-(J11-Pad24)")
      (node (ref J11) (pin 24)))
    (net (code 249) (name "Net-(J11-Pad26)")
      (node (ref J11) (pin 26)))
    (net (code 250) (name "Net-(J11-Pad31)")
      (node (ref J11) (pin 31)))
    (net (code 251) (name "Net-(J11-Pad29)")
      (node (ref J11) (pin 29)))
    (net (code 252) (name "Net-(J11-Pad7)")
      (node (ref J11) (pin 7)))
    (net (code 253) (name "Net-(J11-Pad5)")
      (node (ref J11) (pin 5)))
    (net (code 254) (name "Net-(J11-Pad3)")
      (node (ref J11) (pin 3)))
    (net (code 255) (name "Net-(J10-Pad3)")
      (node (ref J10) (pin 3)))
    (net (code 256) (name "Net-(J16-Pad3)")
      (node (ref J16) (pin 3))
      (node (ref JP21) (pin 2)))
    (net (code 257) (name "Net-(JP20-Pad1)")
      (node (ref JP20) (pin 1)))
    (net (code 258) (name "Net-(JP21-Pad1)")
      (node (ref JP21) (pin 1)))
    (net (code 259) (name "Net-(J10-Pad1)")
      (node (ref J10) (pin 1)))
    (net (code 260) (name "Net-(J10-Pad2)")
      (node (ref J10) (pin 2)))
    (net (code 261) (name "Net-(J10-Pad4)")
      (node (ref J10) (pin 4)))
    (net (code 262) (name "Net-(J10-Pad5)")
      (node (ref J10) (pin 5)))
    (net (code 263) (name "Net-(J10-Pad6)")
      (node (ref J10) (pin 6)))
    (net (code 264) (name "Net-(J10-Pad7)")
      (node (ref J10) (pin 7)))
    (net (code 265) (name "Net-(J10-Pad8)")
      (node (ref J10) (pin 8)))
    (net (code 266) (name "Net-(J11-Pad10)")
      (node (ref JP12) (pin 2))
      (node (ref J11) (pin 10)))
    (net (code 267) (name "Net-(J11-Pad27)")
      (node (ref J11) (pin 27))
      (node (ref JP13) (pin 1)))
    (net (code 268) (name "Net-(J11-Pad28)")
      (node (ref J11) (pin 28))
      (node (ref JP14) (pin 1)))
    (net (code 269) (name "Net-(J11-Pad11)")
      (node (ref J11) (pin 11)))
    (net (code 270) (name "Net-(J11-Pad12)")
      (node (ref J11) (pin 12)))
    (net (code 271) (name "Net-(J11-Pad35)")
      (node (ref J11) (pin 35)))
    (net (code 272) (name "Net-(J11-Pad38)")
      (node (ref J11) (pin 38)))
    (net (code 273) (name "Net-(J11-Pad40)")
      (node (ref J11) (pin 40)))
    (net (code 274) (name "Net-(J11-Pad15)")
      (node (ref J11) (pin 15)))
    (net (code 275) (name "Net-(J11-Pad16)")
      (node (ref J11) (pin 16)))
    (net (code 276) (name "Net-(J11-Pad18)")
      (node (ref J11) (pin 18)))
    (net (code 277) (name "Net-(J11-Pad22)")
      (node (ref J11) (pin 22)))
    (net (code 278) (name "Net-(J11-Pad37)")
      (node (ref J11) (pin 37)))
    (net (code 279) (name "Net-(J11-Pad13)")
      (node (ref J11) (pin 13)))
    (net (code 280) (name "Net-(J9-Pad6)")
      (node (ref J9) (pin 6)))
    (net (code 281) (name "Net-(J9-Pad2)")
      (node (ref J9) (pin 2)))
    (net (code 282) (name "Net-(J11-Pad36)")
      (node (ref J11) (pin 36)))
    (net (code 283) (name "Net-(J15-Pad1)")
      (node (ref J15) (pin 1))
      (node (ref U13) (pin 7))
      (node (ref R18) (pin 2))
      (node (ref U12) (pin 7)))
    (net (code 284) (name "Net-(U8-Pad7)")
      (node (ref U8) (pin 7)))
    (net (code 285) (name "Net-(U8-Pad3)")
      (node (ref U8) (pin 3)))
    (net (code 286) (name "Net-(U8-Pad2)")
      (node (ref U8) (pin 2)))
    (net (code 287) (name "Net-(U8-Pad1)")
      (node (ref U8) (pin 1)))
    (net (code 288) (name "Net-(U9-Pad7)")
      (node (ref U9) (pin 7)))
    (net (code 289) (name "Net-(J7-Pad1)")
      (node (ref R13) (pin 2))
      (node (ref U6) (pin 7))
      (node (ref U7) (pin 7))
      (node (ref J7) (pin 1)))
    (net (code 290) (name "Net-(U9-Pad1)")
      (node (ref U9) (pin 1)))
    (net (code 291) (name "Net-(U9-Pad2)")
      (node (ref U9) (pin 2)))
    (net (code 292) (name "Net-(U9-Pad3)")
      (node (ref U9) (pin 3)))))
